|  |
| --- |
|  |

|  |  |
| --- | --- |
| CHANGE REQUEST | |
| Meeting ID:\* | SDS 40 |
| Source:\* | Bob Flynn, Convida Wireless , Bob.Flynn@convidawireless.com |
| Date:\* | 2019-05-20 |
| Reason for Change/s:\* | correction |
| CR against: Release\* | Rel-4 |
| CR against: WI\* | Active <Work Item number>  MNT maintenance / < Work Item number(optional)>  Is this a mirror CR? Yes  No  mirror CR number: (Note to Rapporteur - use latest agreed revision)  STE Small Technical Enhancements / < Work Item number (optional)>  Only ONE of the above shall be ticked |
| CR against: TS/TR\* | TS-0001 v4.0.0 |
| Clauses \* | 9.6.36 |
| Type of change: \* | Editorial change  Bug Fix or Correction  Change to existing feature or functionality  New feature or functionality  Only ONE of the above shall be ticked |
| Other TS/TR(s) impacted | None |
| Post Freeze checking:\* | This CR contains only essential changes and corrections? YES  NO  This CR may break backwards compatibility with the last approved version of the TS? YES  NO |
| Template Version: January 2019 (do not modify) | |

**oneM2M Notice**

The document to which this cover statement is attached is submitted to oneM2M. Participation in, or attendance at, any activity of oneM2M, constitutes acceptance of and agreement to be bound by terms of the Working Procedures and the Partnership Agreement, including the Intellectual Property Rights (IPR) Principles Governing oneM2M Work found in Annex 1 of the Partnership Agreement.

GUIDELINES for Change Requests:

Provide an informative introduction containing the problem(s) being solved, and a summary list of proposals.

Each CR should contain changes related to only one particular issue/problem.

In case of a correction, and the change apply to previous releases, a separate “mirror CR” should be posted at the same time of this CR

Mirror CR: applies only when the text, including clause numbering are exactly the same.

Companion CR: applies when the change means the same but the baselines differ in some way (e.g. clause number).

Follow the principle of completeness, where all changes related to the issue or problem within a deliverable are simultaneously proposed to be made E.g. A change impacting 5 tables should not only include a proposal to change only 3 tables. Includes any changes to references, definitions, and acronyms in the same deliverable.

Follow the drafting rules.

All pictures must be editable.

Check spelling and grammar to the extent practicable.

Use Change bars for modifications.

The change should include the current and surrounding clauses to clearly show where a change is located and to provide technical context of the proposed change. Additions of complete clauses need not show surrounding clauses as long as the proposed clause number clearly shows where the new clause is proposed to be located.

Multiple changes in a single CR shall be clearly separated by horizontal lines with embedded text such as, start of change 1, end of change 1, start of new clause, end of new clause.

When subsequent changes are made to content of a CR, then the accepted version should not show changes over changes. The accepted version of the CR should only show changes relative to the baseline approved text.

## Introduction

* Wrong resource name of time series functionality

In the table for attributes of *<timeSeries>*, for the attribute *maxByteSize*, in the description, specification wrongly mentions as *<timeSeriesInstance>* instead of <timeSeries>.

-------------------------------------------------- Start of Change 1--------------------------------------------------

Table 9.6.36-2: Attributes of <*timeSeries*> resource

| Attributes of  *<timeSeries>* | Multiplicity | RW/  RO/  WO | Description | *<timeSeriesAnnc>* Attributes |
| --- | --- | --- | --- | --- |
| *resourceType* | 1 | RO | See clause 9.6.1.3. | NA |
| *resourceID* | 1 | RO | See clause 9.6.1.3. | NA |
| *resourceName* | 1 | WO | See clause 9.6.1.3. | NA |
| *parentID* | 1 | RO | See clause 9.6.1.3. | NA |
| *expirationTime* | 1 | RW | See clause 9.6.1.3 | MA |
| *accessControlPolicyIDs* | 0..1 (L) | RW | See clause 9.6.1.3. | MA |
| *labels* | 0..1 (L) | RW | See clause 9.6.1.3. | MA |
| *creationTime* | 1 | RO | See clause 9.6.1.3. | NA |
| *lastModifiedTime* | 1 | RO | See clause 9.6.1.3. | NA |
| *announceTo* | 0..1 (L) | RW | See clause 9.6.1.3. | NA |
| *announcedAttribute* | 0..1 (L) | RW | See clause 9.6.1.3. | NA |
| *dynamicAuthorizationConsultationIDs* | 0..1 (L) | RW | See clause 9.6.1.3. | OA |
| *creator* | 1 | RO | See clause 9.6.1.3. | NA |
| *maxNrOfInstances* | 0..1 | RW | Maximum number of direct child *<timeSeriesInstance>* resources in the <*timeSeries*> resource. | OA |
| *maxByteSize* | 0..1 | RW | Maximum size in bytes of data that is allocated for the *<timeSeries>* resource for all direct child *<timeSeriesInstance>* resources. | OA |
| *maxInstanceAge* | 0..1 | RW | Maximum age of a direct child *<timeSeriesInstance>* resource in the <*timeSeries*> *resource*. The value is expressed in seconds. | OA |
| *currentNrOfInstances* | 1 | RO | Current number of direct child *<timeSeriesInstance>* resource in the <*timeSeries*> resource. It is limited by the *maxNrOfInstances*. The *currentNrOfInstances* attribute of the <timeSeries> resource shall be updated on successful creation or deletion of direct child < *timeSeriesInstance* > resource of <timeSeries > resource. | OA |
| *currentByteSize* | 1 | RO | Current size in bytes of data stored in all direct child *<timeSeriesInstance>* resources of a <*timeSeries*> resource. It is limited by the *maxByteSize*. The *currentByteSize* attribute of the <timeSeries> resource shall be updated on successful creation or deletion of direct child < *timeSeriesInstance* > resource of <timeSeries > resource. | OA |
| *periodicInterval* | 0..1 | WO | If the Time Series Data is periodic, this attribute shall contain the expected amount of time between two instances of Time Series Data. | OA |
| *missingDataDetect* | 0..1 | WO | Indicates whether the Receiver shall detect the missing Time Series Data if it is periodic. | NA |
| *ontologyRef* | 0..1 | RW | A reference (URI) of the ontology used to represent the information that is stored in the child *<timeSeriesInstance>* resources of the present *<timeSeriesData>* resource (see note). | OA |
| *missingDataMaxNr* | 0..1 | RW | Maximum number of entries in the *missingDataList* if the *periodicInterval* is set and the *missingDataDetect* is TRUE. | OA |
| *missingDataList* | 0..1(L) | RO | The list of the *dataGenerationTime* valuerepresenting the missing Time Series Data in descending order by time if the *periodicInterva*l is set and the *missingDataDetect* is TRUE. | OA |
| *missingDataCurrentNr* | 0..1 | RO | Current number of the missing Time Series Data in the *missingDataList*. | OA |
| *missingDataDetectTimer* | 0..1 | RW | The *missingDataDetectTimer* after which a missing Time Series Data shall be considered lost by the hosting CSE. Note that the setting of this value may not apply in certain transports such as TCP, and as such the hosting CSE may reject proposed values or suggest different values. | OA |
| *contentInfo* | 0..1 | WO | This attribute contains information to understand the contents of the *content* attribute of <timeSeriesInstance>. It shall be composed of two mandatory components consisting of an Internet Media Type (as defined in the IETF RFC 6838 [i.36]) and an encoding type. In addition, an optional content security component may also be included. The format of this attribute is defined in oneM2M TS‑0004 [3].  This attribute should be used to represent the content information of the *content* attribute of child <*timeSeriesInstance*> resources so that AEs can understand the content. | OA |
| NOTE: The access to this URI is out of scope of oneM2M. | | | | |

-------------------------------------------------- End of Change 1---------------------------------------------------