|  |
| --- |
|  |

|  |
| --- |
| CHANGE REQUEST |
| Meeting ID:\* |  RDM #58 |
|   | Andreas Kraft, DT, A.Kraft@telekom.de Andreas Neubacher, DT, Andreas.Neubacher@magenta.at Cyrille Bareau, Orange, cyrille.bareau@orange.comMarianne Mohali, Orange, marianne.mohali@orange.com  |
| Date:\* | 2023-02-20 |
| Reason for Change/s:\* | TS-0023 New shortnames |
| CR against: Release\* | Release 4 |
| CR against: WI\* | [ ]  Active WI-xxxx[x]  MNT maintenance / < Work Item number(optional)>Is this a mirror CR? Yes [ ]  No [ ] mirror CR number: (Note to Rapporteur - use latest agreed revision)[ ]  STE Small Technical Enhancements / < Work Item number (optional)>Only ONE of the above shall be ticked |
| CR against: TS/TR\* | TS-0023, V4.12.0 |
| Clauses \* | 6.3.1 ff |
| Type of change: \* | [ ]  Editorial change[x]  Bug Fix or Correction[ ]  Change to existing feature or functionality[ ]  New feature or functionalityOnly ONE of the above shall be ticked |
| Impacted other TS/TR(s) |  |
| Post Freeze checking:\* | This CR contains only essential changes and corrections? YES [x]  NO [ ] This CR may break backwards compatibility with the last approved version of the TS? YES [ ]  NO [x]  |
| Template Version: January 2017 (Do not modify) |

**oneM2M Notice**

The document to which this cover statement is attached is submitted to oneM2M. Participation in, or attendance at, any activity of oneM2M, constitutes acceptance of and agreement to be bound by terms of the Working Procedures and the Partnership Agreement, including the Intellectual Property Rights (IPR) Principles Governing oneM2M Work found in Annex 1 of the Partnership Agreement.

GUIDELINES for Change Requests:

Provide an informative introduction containing the problem(s) being solved, and a summary list of proposals.

Each CR should contain changes related to only one particular issue/problem.

In case of a correction, and the change apply to previous releases, a separate “mirror CR” should be posted at the same time of this CR

Mirror CR: applies only when the text, including clause numbering are exactly the same.

Companion CR: applies when the change means the same but the baselines differ in some way (e.g. clause number).

Follow the principle of completeness, where all changes related to the issue or problem within a deliverable are simultaneously proposed to be made E.g. A change impacting 5 tables should not only include a proposal to change only 3 tables. Includes any changes to references, definitions, and acronyms in the same deliverable.

Follow the drafting rules.

All pictures must be editable.

Check spelling and grammar to the extent practicable.

Use Change bars for modifications.

The change should include the current and surrounding clauses to clearly show where a change is located and to provide technical context of the proposed change. Additions of complete clauses need not show surrounding clauses as long as the proposed clause number clearly shows where the new clause is proposed to be located.

Multiple changes in a single CR shall be clearly separated by horizontal lines with embedded text such as, start of change 1, end of change 1, start of new clause, end of new clause.

When subsequent changes are made to content of a CR, then the accepted version should not show changes over changes. The accepted version of the CR should only show changes relative to the baseline approved text.

Introduction

This CR proposes a new version of the element name to short name mapping in TS-0023, section 6.3.

In addition to 830+ mappings for this release this CR proposes to move the mappings into one single alphabetical ordered table instead of having separate tables for ModuleClasses, DeviceClasses, Actions, Attributes and Properties etc. Since element names are re-used for different classes and objects and because of the sheer number of mappings it is not possible anymore to separate them anymore.

**R01**

Marked clauses 6.3.3 and 6.3.4 as “Void”.

### \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Start of Change 1 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## 6.3 Short names

### 6.3.1 Introduction

XML and JSON representations require the explicit encoding of the names of resource attributes, (in the case of XML) and resource types. Whenever a protocol binding transfers such a name over a oneM2M reference point, it shall use a shortened form of that name. Short names enable payload reduction on involved telecommunication interfaces.

The mapping between the full names and their shortened form is given in the following clause.

### 6.3.2 Element short names

The following Table 6.3.2-1 presents the combined short names for ModuleClasses, DeviceClasses, SubDevices, Actions, and their attributes and properties.

**Table 6.3.2 1: Element short name mappings**

|  |  |  |
| --- | --- | --- |
| **Element Name** | **Occurs In** | **Short Name** |
| absoluteEnergyConsumption | energyConsumption, energyConsumptionAnnc, energyConsumptionInst | abECn |
| absoluteStartTime | timer, timerAnnc, timerInst | abSTe |
| absoluteStopTime | timer, timerAnnc, timerInst | abST0 |
| acousticSensor |  | acoSr |
| acousticStatus | acousticSensor, acousticSensorAnnc, acousticSensorInst | acoSs |
| activate |  | actie |
| activateClockTimer |  | acCTr |
| address | writeIO, writeIOAnnc, writeIOInst, readIO, readIOAnnc, readIOInst | addrs |
| adfStates | autoDocumentFeeder, autoDocumentFeederAnnc, autoDocumentFeederInst | adfSs |
| airConJobMode |  | aCJMe |
| airFlow |  | airFw |
| airPressure | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | airPe |
| airPurifierJobMode |  | aPJMe |
| airQualitySensor |  | aiQSr |
| alarm | barometer, barometerAnnc, barometerInst, motionSensor, motionSensorAnnc, motionSensorInst, smokeSensor, smokeSensorAnnc, smokeSensorInst, waterSensor, waterSensorAnnc, waterSensorInst | alarm |
| alarmSpeaker |  | alaSr |
| alarmStatus | alarmSpeaker, alarmSpeakerAnnc, alarmSpeakerInst | alaSs |
| alarmTimestamp | temperatureAlarm, temperatureAlarmAnnc, temperatureAlarmInst | alaTp |
| algae | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | algae |
| altitude | geoLocation, geoLocationAnnc, geoLocationInst | altie |
| anemometer |  | anemr |
| anionics | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | anios |
| answer |  | answr |
| areaLatitude | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | areLe |
| areaLongitude | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | areL0 |
| areaNwkType | dmAreaNwkInfo, dmAreaNwkInfoAnnc, dmAreaNwkInfoInst | arNTe |
| areaRadius | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | areRs |
| aroh | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | aroh |
| as | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | as |
| atmosphericPressure | barometer, barometerAnnc, barometerInst | atmPe |
| attached | dmCapability, dmCapabilityAnnc, dmCapabilityInst | attad |
| audioVolume |  | audVe |
| autoDocumentFeeder |  | auDFr |
| automode | airFlow, airFlowAnnc, airFlowInst | autoe |
| availableChannels | televisionChannel, televisionChannelAnnc, televisionChannelInst | avaCs |
| availStorage | dmStorage, dmStorageAnnc, dmStorageInst | avaSe |
| backoffTime | periodicalReportConfig, periodicalReportConfigAnnc, periodicalReportConfigInst | bacTe |
| balance | billDeposit, billDepositAnnc, billDepositInst, billWithdrawal, billWithdrawalAnnc, billWithdrawalInst, cashDispenser, cashDispenserAnnc, cashDispenserInst, coinDeposit, coinDepositAnnc, coinDepositInst, prePaidCardReader, prePaidCardReaderAnnc, prePaidCardReaderInst | balae |
| baliseSystemId | baliseTransmissionModule, baliseTransmissionModuleAnnc, baliseTransmissionModuleInst | baSId |
| baliseTransmissionModule | baliseTransmission | baTMe |
| barometer |  | baror |
| barrierDefault | crossingBarrier, crossingBarrierAnnc, crossingBarrierInst | barDt |
| barrierStatus | crossingBarrier, crossingBarrierAnnc, crossingBarrierInst | barSs |
| basalMetabolism | bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst | basMm |
| bath | hotWaterSupply, hotWaterSupplyAnnc, hotWaterSupplyInst | bath |
| battery |  | bat |
| batteryMaterial | battery, batteryAnnc, batteryInst | batMl |
| batteryShape | battery, batteryAnnc, batteryInst | batSe |
| batteryThreshold | battery, batteryAnnc, batteryInst | batTd |
| billDeposit |  | bilDt |
| billingNumber | gasChargingControl, gasChargingControlAnnc, gasChargingControlInst | bilNr |
| billWithdrawal |  | bilWl |
| binaryObject | image | binOt |
| binarySwitch | gasMeterControl, waterMeterControl, brewingSwitch, boilingSwitch | binSh |
| bioElectricalImpedanceAnalysis |  | bEIAs |
| biotoxicity | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | bioty |
| blue | colour, colourAnnc, colourInst | blue |
| bmi | bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst | bmi |
| bod | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | bod |
| bodyCompositionAnalyser |  | boCAr |
| bodyLength | bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst | bodLh |
| bodyWaterMass | bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst | boWMs |
| boiler |  | boilr |
| bone | bioElectricalImpedanceAnalysis, bioElectricalImpedanceAnalysisAnnc, bioElectricalImpedanceAnalysisInst | bone |
| brewing |  | brewg |
| brightness | brightnessAnnc, brightnessInst, crossingIndicatorColourBrightness | brigs |
| buttonFault | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | butFt |
| call |  | call |
| callerID | phoneCall, phoneCallAnnc, phoneCallInst | calID |
| callState | phoneCall, phoneCallAnnc, phoneCallInst | calSe |
| cancel |  | cancl |
| capacity | battery, batteryAnnc, batteryInst | capay |
| cardInfo | cardScanner, cardScannerAnnc, cardScannerInst, prePaidCardReader, prePaidCardReaderAnnc, prePaidCardReaderInst | carIo |
| cardScanner |  | carSr |
| cashDispenser |  | casDr |
| cd | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | cd |
| cellID | connectivity, connectivityAnnc, connectivityInst | celID |
| certainty | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | certy |
| ch2o | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | ch2o |
| channelName | televisionChannel, televisionChannelAnnc, televisionChannelInst | chaNe |
| channelNumber | televisionChannel, televisionChannelAnnc, televisionChannelInst | chaNr |
| charging | battery, batteryAnnc, batteryInst | charg |
| chargingAmpere | battery, batteryAnnc, batteryInst | chaAe |
| chargingCapacity | electricVehicleConnector, electricVehicleConnectorAnnc, electricVehicleConnectorInst | chaCy |
| chargingVoltage | battery, batteryAnnc, batteryInst | chaVe |
| chlorophyll\_a | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | chloa |
| clock |  | clock |
| close |  | close |
| clothesDryerJobMode |  | cDJMe |
| clothesWasherDryerJobMode |  | cWDJM |
| clothesWasherJobMode |  | cWJMe |
| clothesWasherJobModeOption |  | cWJMO |
| cn | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | cn |
| co | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | co |
| co2 | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | co2 |
| coarseness | grinder, grinderAnnc, grinderInst | coars |
| cod | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | cod |
| code | faultDetection, faultDetectionAnnc, faultDetectionInst | code |
| coinDeposit |  | coiDt |
| coldWash | clothesWasherJobModeOption, clothesWasherJobModeOptionAnnc, clothesWasherJobModeOptionInst | colWh |
| colour | crossingIndicatorColour | color |
| colourSaturation | colourSaturationAnnc, colourSaturationInst, crossingIndicatorColourSaturation | colSn |
| colourTemperature | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | colTe |
| commFreqValue | connectivity, connectivityAnnc, connectivityInst | coFVe |
| communicationAlarm | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | comAm |
| component | dmFirmware, dmFirmwareAnnc, dmFirmwareInst | compt |
| concentration | glucometer, glucometerAnnc, glucometerInst | concn |
| conductivity | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | condy |
| connectivity |  | conny |
| contextCarbohydratesAmount | glucometer, glucometerAnnc, glucometerInst | coCAt |
| contextCarbohydratesSource | glucometer, glucometerAnnc, glucometerInst | coCSe |
| contextExercise | glucometer, glucometerAnnc, glucometerInst | conEe |
| contextHealth | glucometer, glucometerAnnc, glucometerInst | conHh |
| contextLocation | glucometer, glucometerAnnc, glucometerInst | conLn |
| contextMeal | glucometer, glucometerAnnc, glucometerInst | conMl |
| contextMedication | glucometer, glucometerAnnc, glucometerInst | conMn |
| contextTester | glucometer, glucometerAnnc, glucometerInst | conTr |
| cookerHoodJobMode |  | cHJMe |
| count | billDeposit, billDepositAnnc, billDepositInst, billWithdrawal, billWithdrawalAnnc, billWithdrawalInst, cashDispenser, cashDispenserAnnc, cashDispenserInst, coinDeposit, coinDepositAnnc, coinDepositInst | count |
| country | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst | couny |
| cowActivityMonitor |  | coAMr |
| cpuUsage | dmAgent, dmAgentAnnc, dmAgentInst | cpuUe |
| cr6 | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | cr6 |
| credentials |  | creds |
| crossingBarrier |  | croBr |
| cu | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | cu |
| cumulativeFlow | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | cumFw |
| cumulativeFlowDaily | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | cuFDy |
| cupsNumber | brewing, brewingAnnc, brewingInst | cupNr |
| currency | billDeposit, billDepositAnnc, billDepositInst, cashDispenser, cashDispenserAnnc, cashDispenserInst, coinDeposit, coinDepositAnnc, coinDepositInst, prePaidCardReader, prePaidCardReaderAnnc, prePaidCardReaderInst | curry |
| current | energyConsumption, energyConsumptionAnnc, energyConsumptionInst | currt |
| currentAdfState | autoDocumentFeeder, autoDocumentFeederAnnc, autoDocumentFeederInst | cuASe |
| currentCycleBeginn | connectivity, connectivityAnnc, connectivityInst | cuCBn |
| currentCycleTransmissionErrors | connectivity, connectivityAnnc, connectivityInst | cCTEs |
| currentCycleVolume | connectivity, connectivityAnnc, connectivityInst | cuCVe |
| currentDate | clock, clockAnnc, clockInst | curDe |
| currentJobMode | airConJobMode, airConJobModeAnnc, airConJobModeInst, airPurifierJobMode, airPurifierJobModeAnnc, airPurifierJobModeInst, clothesDryerJobMode, clothesDryerJobModeAnnc, clothesDryerJobModeInst, clothesWasherDryerJobMode, clothesWasherDryerJobModeAnnc, clothesWasherDryerJobModeInst, clothesWasherJobMode, clothesWasherJobModeAnnc, clothesWasherJobModeInst, cookerHoodJobMode, cookerHoodJobModeAnnc, cookerHoodJobModeInst, dehumidifierJobMode, dehumidifierJobModeAnnc, dehumidifierJobModeInst, dishWasherJobMode, dishWasherJobModeAnnc, dishWasherJobModeInst, robotCleanerJobMode, robotCleanerJobModeAnnc, robotCleanerJobModeInst, steamClosetJobMode, steamClosetJobModeAnnc, steamClosetJobModeInst | cuJMe |
| currentJobModeName | airConJobMode, airConJobModeAnnc, airConJobModeInst, airPurifierJobMode, airPurifierJobModeAnnc, airPurifierJobModeInst, clothesDryerJobMode, clothesDryerJobModeAnnc, clothesDryerJobModeInst, clothesWasherDryerJobMode, clothesWasherDryerJobModeAnnc, clothesWasherDryerJobModeInst, clothesWasherJobMode, clothesWasherJobModeAnnc, clothesWasherJobModeInst, cookerHoodJobMode, cookerHoodJobModeAnnc, cookerHoodJobModeInst, dehumidifierJobMode, dehumidifierJobModeAnnc, dehumidifierJobModeInst, dishWasherJobMode, dishWasherJobModeAnnc, dishWasherJobModeInst, robotCleanerJobMode, robotCleanerJobModeAnnc, robotCleanerJobModeInst, steamClosetJobMode, steamClosetJobModeAnnc, steamClosetJobModeInst | cJMNe |
| currentJobState | runState, runStateAnnc, runStateInst | cuJSe |
| currentMachineState | runState, runStateAnnc, runStateInst | cuMSe |
| currentPlayerMode | playerControl, playerControlAnnc, playerControlInst | cuPMe |
| currentPlayerModeName | playerControl, playerControlAnnc, playerControlInst | cPMNe |
| currentSecurityMode | securityMode, securityModeAnnc, securityModeInst | cuSMe |
| currentState | dmCapability, dmCapabilityAnnc, dmCapabilityInst | curSe |
| currentTemperature | temperature, temperatureAnnc, temperatureInst | curT0 |
| currentTime | clock, clockAnnc, clockInst | curTe |
| currentTimeZone | clock, clockAnnc, clockInst | cuTZe |
| currentValue | smokeSensor, smokeSensorAnnc, smokeSensorInst | crv |
| dailyActivityTime | connectivity, connectivityAnnc, connectivityInst | daATe |
| dailyNumberOfConnections | connectivity, connectivityAnnc, connectivityInst | dNOCs |
| dailyUseWaterTime | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | dUWTe |
| data | dmEventLog, dmEventLogAnnc, dmEventLogInst | data |
| dataGenerationTime | threeDDisplay, threeDDisplayAnnc, threeDDisplayInst, threeDPrinter, threeDPrinterAnnc, threeDPrinterInst, threeDScanner, threeDScannerAnnc, threeDScannerInst, acousticSensor, acousticSensorAnnc, acousticSensorInst, airConJobMode, airConJobModeAnnc, airConJobModeInst, airFlow, airFlowAnnc, airFlowInst, airPurifierJobMode, airPurifierJobModeAnnc, airPurifierJobModeInst, airQualitySensor, airQualitySensorAnnc, airQualitySensorInst, alarmSpeaker, alarmSpeakerAnnc, alarmSpeakerInst, anemometer, anemometerAnnc, anemometerInst, audioVolume, audioVolumeAnnc, audioVolumeInst, autoDocumentFeeder, autoDocumentFeederAnnc, autoDocumentFeederInst, barometer, barometerAnnc, barometerInst, battery, batteryAnnc, batteryInst, billDeposit, billDepositAnnc, billDepositInst, billWithdrawal, billWithdrawalAnnc, billWithdrawalInst, binaryObject, binaryObjectAnnc, binaryObjectInst, binarySwitch, binarySwitchAnnc, binarySwitchInst, bioElectricalImpedanceAnalysis, bioElectricalImpedanceAnalysisAnnc, bioElectricalImpedanceAnalysisInst, bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst, boiler, boilerAnnc, boilerInst, brewing, brewingAnnc, brewingInst, brightness, brightnessAnnc, brightnessInst, cardScanner, cardScannerAnnc, cardScannerInst, cashDispenser, cashDispenserAnnc, cashDispenserInst, clock, clockAnnc, clockInst, clothesDryerJobMode, clothesDryerJobModeAnnc, clothesDryerJobModeInst, clothesWasherDryerJobMode, clothesWasherDryerJobModeAnnc, clothesWasherDryerJobModeInst, clothesWasherJobMode, clothesWasherJobModeAnnc, clothesWasherJobModeInst, clothesWasherJobModeOption, clothesWasherJobModeOptionAnnc, clothesWasherJobModeOptionInst, coinDeposit, coinDepositAnnc, coinDepositInst, colour, colourAnnc, colourInst, colourSaturation, colourSaturationAnnc, colourSaturationInst, connectivity, connectivityAnnc, connectivityInst, cookerHoodJobMode, cookerHoodJobModeAnnc, cookerHoodJobModeInst, credentials, credentialsAnnc, credentialsInst, crossingBarrier, crossingBarrierAnnc, crossingBarrierInst, dehumidifierJobMode, dehumidifierJobModeAnnc, dehumidifierJobModeInst, dishWasherJobMode, dishWasherJobModeAnnc, dishWasherJobModeInst, disposal, disposalAnnc, disposalInst, doorStatus, doorStatusAnnc, doorStatusInst, electricVehicleConnector, electricVehicleConnectorAnnc, electricVehicleConnectorInst, energyConsumption, energyConsumptionAnnc, energyConsumptionInst, energyGeneration, energyGenerationAnnc, energyGenerationInst, faultDetection, faultDetectionAnnc, faultDetectionInst, filterInfo, filterInfoAnnc, filterInfoInst, foaming, foamingAnnc, foamingInst, galleryMode, galleryModeAnnc, galleryModeInst, gasChargingControl, gasChargingControlAnnc, gasChargingControlInst, gasMeterAlarm, gasMeterAlarmAnnc, gasMeterAlarmInst, gasMeterReportInfo, gasMeterReportInfoAnnc, gasMeterReportInfoInst, geoLocation, geoLocationAnnc, geoLocationInst, glucometer, glucometerAnnc, glucometerInst, grinder, grinderAnnc, grinderInst, headingSensor, headingSensorAnnc, headingSensorInst, heatingZone, heatingZoneAnnc, heatingZoneInst, height, heightAnnc, heightInst, hotWaterSupply, hotWaterSupplyAnnc, hotWaterSupplyInst, impactSensor, impactSensorAnnc, impactSensorInst, infraredSensor, infraredSensorAnnc, infraredSensorInst, keepWarm, keepWarmAnnc, keepWarmInst, keypad, keypadAnnc, keypadInst, liquidLevel, liquidLevelAnnc, liquidLevelInst, liquidRemaining, liquidRemainingAnnc, liquidRemainingInst, lock, lockAnnc, lockInst, magneticSensorParameters, magneticSensorParametersAnnc, magneticSensorParametersInst, mediaSelect, mediaSelectAnnc, mediaSelectInst, motionSensor, motionSensorAnnc, motionSensorInst, numberValue, numberValueAnnc, numberValueInst, openLevel, openLevelAnnc, openLevelInst, operationMode, operationModeAnnc, operationModeInst, overcurrentSensor, overcurrentSensorAnnc, overcurrentSensorInst, oximeter, oximeterAnnc, oximeterInst, ozoneMeter, ozoneMeterAnnc, ozoneMeterInst, parkingStatus, parkingStatusAnnc, parkingStatusInst, periodicalReportConfig, periodicalReportConfigAnnc, periodicalReportConfigInst, phoneCall, phoneCallAnnc, phoneCallInst, playerControl, playerControlAnnc, playerControlInst, powerSave, powerSaveAnnc, powerSaveInst, prePaidCardReader, prePaidCardReaderAnnc, prePaidCardReaderInst, printQueue, printQueueAnnc, printQueueInst, pulsemeter, pulsemeterAnnc, pulsemeterInst, pushButton, pushButtonAnnc, pushButtonInst, rainGauge, rainGaugeAnnc, rainGaugeInst, recorder, recorderAnnc, recorderInst, refrigeration, refrigerationAnnc, refrigerationInst, relativeHumidity, relativeHumidityAnnc, relativeHumidityInst, remoteControlEnable, remoteControlEnableAnnc, remoteControlEnableInst, robotCleanerJobMode, robotCleanerJobModeAnnc, robotCleanerJobModeInst, runState, runStateAnnc, runStateInst, securityMode, securityModeAnnc, securityModeInst, sessionDescription, sessionDescriptionAnnc, sessionDescriptionInst, signalPanel, signalPanelAnnc, signalPanelInst, signalStrength, signalStrengthAnnc, signalStrengthInst, slcAlarm, slcAlarmAnnc, slcAlarmInst, slcParameterSetting, slcParameterSettingAnnc, slcParameterSettingInst, slcReportInfo, slcReportInfoAnnc, slcReportInfoInst, smokeSensor, smokeSensorAnnc, smokeSensorInst, sphygmomanometer, sphygmomanometerAnnc, sphygmomanometerInst, spinLevel, spinLevelAnnc, spinLevelInst, steamClosetJobMode, steamClosetJobModeAnnc, steamClosetJobModeInst, televisionChannel, televisionChannelAnnc, televisionChannelInst, temperature, temperatureAnnc, temperatureInst, temperatureAlarm, temperatureAlarmAnnc, temperatureAlarmInst, textMessage, textMessageAnnc, textMessageInst, timer, timerAnnc, timerInst, turbo, turboAnnc, turboInst, touchScreen, touchScreenAnnc, touchScreenInst, uvSensor, uvSensorAnnc, uvSensorInst, waterFilterType, waterFilterTypeAnnc, waterFilterTypeInst, waterFlow, waterFlowAnnc, waterFlowInst, waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst, waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst, waterMeterSetting, waterMeterSettingAnnc, waterMeterSettingInst, waterSensor, waterSensorAnnc, waterSensorInst, waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst, weight, weightAnnc, weightInst, unmuteAudioVolume, unmuteAudioVolumeAnnc, unmuteAudioVolumeInst, resetTextMessage, resetTextMessageAnnc, resetTextMessageInst, reset, resetAnnc, resetInst, activateClockTimer, activateClockTimerAnnc, activateClockTimerInst, nextTrack, nextTrackAnnc, nextTrackInst, deactivateClockTimer, deactivateClockTimerAnnc, deactivateClockTimerInst, previousTrack, previousTrackAnnc, previousTrackInst, upChannel, upChannelAnnc, upChannelInst, start3Dprint, start3DprintAnnc, start3DprintInst, decrementNumberValue, decrementNumberValueAnnc, decrementNumberValueInst, open, openAnnc, openInst, downChannel, downChannelAnnc, downChannelInst, stop3Dprint, stop3DprintAnnc, stop3DprintInst, incrementNumberValue, incrementNumberValueAnnc, incrementNumberValueInst, close, closeAnnc, closeInst, call, callAnnc, callInst, resetNumberValue, resetNumberValueAnnc, resetNumberValueInst, answer, answerAnnc, answerInst, hangup, hangupAnnc, hangupInst, mute, muteAnnc, muteInst, test, testAnnc, testInst, toggle, toggleAnnc, toggleInst, upVolume, upVolumeAnnc, upVolumeInst, downVolume, downVolumeAnnc, downVolumeInst, muteAudioVolume, muteAudioVolumeAnnc, muteAudioVolumeInst, cowActivityMonitor, cowActivityMonitorAnnc, cowActivityMonitorInst, dmAgent, dmAgentAnnc, dmAgentInst, dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst, dmDataModelIO, dmDataModelIOAnnc, dmDataModelIOInst, dmFirmware, dmFirmwareAnnc, dmFirmwareInst, dmSoftware, dmSoftwareAnnc, dmSoftwareInst, dmEventLog, dmEventLogAnnc, dmEventLogInst, dmPackage, dmPackageAnnc, dmPackageInst, dmAreaNwkDeviceInfo, dmAreaNwkDeviceInfoAnnc, dmAreaNwkDeviceInfoInst, dmCapability, dmCapabilityAnnc, dmCapabilityInst, dmStorage, dmStorageAnnc, dmStorageInst, deployPackage, deployPackageAnnc, deployPackageInst, writeIO, writeIOAnnc, writeIOInst, updateFirmware, updateFirmwareAnnc, updateFirmwareInst, disable, disableAnnc, disableInst, update, updateAnnc, updateInst, enable, enableAnnc, enableInst, activate, activateAnnc, activateInst, retrieveLog, retrieveLogAnnc, retrieveLogInst, install, installAnnc, installInst, format, formatAnnc, formatInst, reboot, rebootAnnc, rebootInst, deactivate, deactivateAnnc, deactivateInst, unmount, unmountAnnc, unmountInst, uninstall, uninstallAnnc, uninstallInst, readIO, readIOAnnc, readIOInst, features, featuresAnnc, featuresInst, location, locationAnnc, locationInst, localization, localizationAnnc, localizationInst, origin, originAnnc, originInst, baliseTransmissionModule, baliseTransmissionModuleAnnc, baliseTransmissionModuleInst, disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst, settings, settingsAnnc, settingsInst, cancel, cancelAnnc, cancelInst | dgt |
| dataModelType | dmDataModelIO, dmDataModelIOAnnc, dmDataModelIOInst | daMTe |
| dataSourceID | origin, originAnnc, originInst | daSID |
| dataType | origin, originAnnc, originInst | datTe |
| deactivate |  | deace |
| deactivateClockTimer |  | deCTr |
| decrementNumberValue |  | deNVe |
| defaultValue | numberValue, numberValueAnnc, numberValueInst, textMessage, textMessageAnnc, textMessageInst | defVe |
| defrost | refrigeration, refrigerationAnnc, refrigerationInst | defrt |
| degerm | refrigeration, refrigerationAnnc, refrigerationInst | degem |
| dehumidifierJobMode |  | deJMe |
| demolitionAlarm | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | demAm |
| deodorize | refrigeration, refrigerationAnnc, refrigerationInst | deode |
| deployPackage |  | depPe |
| depositStatus | billDeposit, billDepositAnnc, billDepositInst, coinDeposit, coinDepositAnnc, coinDepositInst | depSs |
| description | faultDetection, faultDetectionAnnc, faultDetectionInst, dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst, localization, localizationAnnc, localizationInst | dc |
| desiredHumidity | relativeHumidity, relativeHumidityAnnc, relativeHumidityInst | desHy |
| detectedTime | infraredSensor, infraredSensorAnnc, infraredSensorInst, overcurrentSensor, overcurrentSensorAnnc, overcurrentSensorInst, smokeSensor, smokeSensorAnnc, smokeSensorInst | detTe |
| detectedValue | infraredSensor, infraredSensorAnnc, infraredSensorInst | detVe |
| detectionInterval | magneticSensorParameters, magneticSensorParametersAnnc, magneticSensorParametersInst | detIl |
| device3DDisplay |  | deDDy |
| device3DPrinter |  | deDPr |
| device3DScanner |  | deDSr |
| deviceAirConditioner |  | deACr |
| deviceAirPurifier |  | deAPr |
| deviceAirQualityMonitor |  | dAQMr |
| deviceAudioReceiver |  | deARr |
| deviceBloodPressureMonitor |  | dBPMr |
| deviceBottleWarmer |  | deBWr |
| deviceCamera |  | devCa |
| deviceCardRechargingMachine |  | dCRMe |
| deviceClothesDryer |  | deCDr |
| deviceClothesWasher |  | deCWr |
| deviceClothesWasherDryer |  | dCWDr |
| deviceCoffeeMachine |  | deCMe |
| deviceCookerHood |  | deCHd |
| deviceCooktop |  | devCp |
| deviceCowActivityMonitor |  | dCAMr |
| deviceDehumidifier |  | devDr |
| deviceDigitalGallery |  | deDGy |
| deviceDishWasher |  | deDWr |
| deviceDoor |  | devD0 |
| deviceDoorLock |  | deDLk |
| deviceElectricVehicleCharger |  | dEVCr |
| deviceFan |  | devFn |
| deviceFoodProbe |  | deFPe |
| deviceFreezer |  | devFr |
| deviceGarbageDisposal |  | deGDp |
| deviceGenericSensor |  | deGSr |
| deviceGlucosemeter |  | devGr |
| deviceHandheldPTTTerminal |  | dHPTT |
| deviceHeartRateMonitor |  | dHRMr |
| deviceHomeCCTV |  | dHCCT |
| deviceHumidifier |  | devHr |
| deviceKettle |  | devKe |
| deviceLight |  | devLt |
| deviceMagneticParkingMonitor |  | dMPMr |
| deviceMicrogeneration |  | devMn |
| deviceMultiFunctionPrinter |  | dMFPr |
| deviceOutdoorLamp |  | deOLp |
| deviceOven |  | devOn |
| devicePrinter |  | devPr |
| devicePulseOximeter |  | dePOr |
| devicePWSCenter |  | dPWSC |
| devicePWSEquipment |  | dPWSE |
| deviceRefrigerator |  | devRr |
| deviceRiceCooker |  | deRC0 |
| deviceRobotCleaner |  | deRCr |
| deviceScanner |  | devSr |
| deviceSecurityPanel |  | deSPl |
| deviceServiceButton |  | deSBn |
| deviceSetTopBox |  | dSTBx |
| deviceSmartElectricMeter |  | dSEMr |
| deviceSmartGasMeter |  | dSGMr |
| deviceSmartGate |  | deSGe |
| deviceSmartPlug |  | deSPg |
| deviceSmartScreenDoor |  | dSSDr |
| deviceSmartWaterMeter |  | dSWMr |
| deviceSteamCloset |  | deSCt |
| deviceStorageBattery |  | deSBy |
| deviceStreetLightController |  | dSLCr |
| deviceSwitch |  | devSh |
| deviceTelevision |  | devTn |
| deviceThermometer |  | devTr |
| deviceThermostat |  | devTt |
| deviceTrainborneTerminal |  | deTTl |
| deviceWaterHeater |  | deWHr |
| deviceWaterPurifier |  | deWPr |
| deviceWaterQualityMonitor |  | dWQMr |
| deviceWaterValve |  | deWVe |
| deviceWeatherStation |  | deWSn |
| deviceWeightScaleAndBodyCompositionAnalyser |  | dWSAB |
| deviceWindowShade |  | deWSe |
| devId | dmAreaNwkDeviceInfo, dmAreaNwkDeviceInfoAnnc, dmAreaNwkDeviceInfoInst | devId |
| devType | dmAreaNwkDeviceInfo, dmAreaNwkDeviceInfoAnnc, dmAreaNwkDeviceInfoInst | devTe |
| diastolicPressure | sphygmomanometer, sphygmomanometerAnnc, sphygmomanometerInst | diaPe |
| disable |  | disae |
| discharging | battery, batteryAnnc, batteryInst | discg |
| dischargingAmpere | battery, batteryAnnc, batteryInst | disAe |
| dischargingCapacity | electricVehicleConnector, electricVehicleConnectorAnnc, electricVehicleConnectorInst | disCy |
| dischargingVoltage | battery, batteryAnnc, batteryInst | disVe |
| dishWasherJobMode |  | dWJMe |
| dismantled | smokeSensor, smokeSensorAnnc, smokeSensorInst | dismd |
| dispenseStatus | cashDispenser, cashDispenserAnnc, cashDispenserInst | disSs |
| displayInterval | galleryMode, galleryModeAnnc, galleryModeInst | disIl |
| displayOrder | galleryMode, galleryModeAnnc, galleryModeInst | disOr |
| displayOrientation | galleryMode, galleryModeAnnc, galleryModeInst | disOn |
| disposal |  | displ |
| disposalStatus | disposal, disposalAnnc, disposalInst | disS0 |
| disseminator |  | dissr |
| dmAgent |  | dmAgt |
| dmAreaNwkDeviceInfo |  | dANDo |
| dmAreaNwkInfo |  | dANIo |
| dmCapability |  | dmCay |
| dmDataModelIO |  | dDMIO |
| dmDeviceInfo |  | dmDIo |
| dmEventLog |  | dmELg |
| dmFirmware |  | dmFie |
| dmPackage |  | dmPae |
| dmSoftware |  | dmSoe |
| dmStorage |  | dmSte |
| do | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | do |
| doorState | doorStatus, doorStatusAnnc, doorStatusInst | dooSe |
| doorStatus |  | dooSs |
| downChannel |  | dowCl |
| downVolume |  | dowVe |
| duration | overcurrentSensor, overcurrentSensorAnnc, overcurrentSensorInst, recorder, recorderAnnc, recorderInst | dur |
| effective | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | effee |
| electricVehicleConnector |  | elVCr |
| emergencyHandler |  | emeHr |
| emergencyMode | emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | emeMe |
| enable |  | enabe |
| enabled | dmEventLog, dmEventLogAnnc, dmEventLogInst | enabd |
| end | retrieveLog, retrieveLogAnnc, retrieveLogInst | end |
| energy | pulsemeter, pulsemeterAnnc, pulsemeterInst | enery |
| energyConsumption | touchscreen | eneCn |
| energyGeneration |  | eneGn |
| estimatedTimeToEnd | timer, timerAnnc, timerInst | eTTEd |
| eventCodes | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | eveCs |
| expires | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | expis |
| extraRinse | clothesWasherJobModeOption, clothesWasherJobModeOptionAnnc, clothesWasherJobModeOptionInst | extRe |
| f | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | f |
| fakeStatus | billDeposit, billDepositAnnc, billDepositInst, coinDeposit, coinDepositAnnc, coinDepositInst | fakSs |
| fat | bioElectricalImpedanceAnalysis, bioElectricalImpedanceAnalysisAnnc, bioElectricalImpedanceAnalysisInst | fat |
| fatFreeMass | bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst | faFMs |
| faultDetection |  | fauDn |
| fe | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | fe |
| features |  | feats |
| fileSystem | dmStorage, dmStorageAnnc, dmStorageInst | filSm |
| filterInfo | waterFilterInfo | filIo |
| filterLifetime | filterInfo, filterInfoAnnc, filterInfoInst | filLe |
| filterType | waterFilterType, waterFilterTypeAnnc, waterFilterTypeInst | filTe |
| flexNode |  | fleNe |
| flexNodeLink | device3DPrinter, device3DPrinterAnnc, device3DPrinterInst, deviceAirQualityMonitor, deviceAirQualityMonitorAnnc, deviceAirQualityMonitorInst, deviceAudioReceiver, deviceAudioReceiverAnnc, deviceAudioReceiverInst, deviceCamera, deviceCameraAnnc, deviceCameraInst, deviceDoor, deviceDoorAnnc, deviceDoorInst, deviceDoorLock, deviceDoorLockAnnc, deviceDoorLockInst, deviceGenericSensor, deviceGenericSensorAnnc, deviceGenericSensorInst, deviceLight, deviceLightAnnc, deviceLightInst, deviceMultiFunctionPrinter, deviceMultiFunctionPrinterAnnc, deviceMultiFunctionPrinterInst, devicePrinter, devicePrinterAnnc, devicePrinterInst, deviceScanner, deviceScannerAnnc, deviceScannerInst, deviceServiceButton, deviceServiceButtonAnnc, deviceServiceButtonInst, deviceSmartPlug, deviceSmartPlugAnnc, deviceSmartPlugInst, deviceSwitch, deviceSwitchAnnc, deviceSwitchInst, deviceThermometer, deviceThermometerAnnc, deviceThermometerInst, deviceThermostat, deviceThermostatAnnc, deviceThermostatInst, deviceWaterValve, deviceWaterValveAnnc, deviceWaterValveInst, device3DDisplay, device3DDisplayAnnc, device3DDisplayInst, device3DScanner, device3DScannerAnnc, device3DScannerInst, deviceCowActivityMonitor, deviceCowActivityMonitorAnnc, deviceCowActivityMonitorInst, deviceOutdoorLamp, deviceOutdoorLampAnnc, deviceOutdoorLampInst, deviceMagneticParkingMonitor, deviceMagneticParkingMonitorAnnc, deviceMagneticParkingMonitorInst, deviceSmartElectricMeter, deviceSmartElectricMeterAnnc, deviceSmartElectricMeterInst, deviceSmartGasMeter, deviceSmartGasMeterAnnc, deviceSmartGasMeterInst, deviceSmartWaterMeter, deviceSmartWaterMeterAnnc, deviceSmartWaterMeterInst, deviceStreetLightController, deviceStreetLightControllerAnnc, deviceStreetLightControllerInst, deviceWaterQualityMonitor, deviceWaterQualityMonitorAnnc, deviceWaterQualityMonitorInst, deviceWeatherStation, deviceWeatherStationAnnc, deviceWeatherStationInst, deviceBloodPressureMonitor, deviceBloodPressureMonitorAnnc, deviceBloodPressureMonitorInst, deviceGlucosemeter, deviceGlucosemeterAnnc, deviceGlucosemeterInst, deviceHeartRateMonitor, deviceHeartRateMonitorAnnc, deviceHeartRateMonitorInst, devicePulseOximeter, devicePulseOximeterAnnc, devicePulseOximeterInst, deviceWeightScaleAndBodyCompositionAnalyser, deviceWeightScaleAndBodyCompositionAnalyserAnnc, deviceWeightScaleAndBodyCompositionAnalyserInst, deviceAirConditioner, deviceAirConditionerAnnc, deviceAirConditionerInst, deviceAirPurifier, deviceAirPurifierAnnc, deviceAirPurifierInst, deviceBottleWarmer, deviceBottleWarmerAnnc, deviceBottleWarmerInst, deviceClothesDryer, deviceClothesDryerAnnc, deviceClothesDryerInst, deviceClothesWasher, deviceClothesWasherAnnc, deviceClothesWasherInst, deviceClothesWasherDryer, deviceClothesWasherDryerAnnc, deviceClothesWasherDryerInst, deviceCoffeeMachine, deviceCoffeeMachineAnnc, deviceCoffeeMachineInst, deviceCookerHood, deviceCookerHoodAnnc, deviceCookerHoodInst, deviceCooktop, deviceCooktopAnnc, deviceCooktopInst, deviceDehumidifier, deviceDehumidifierAnnc, deviceDehumidifierInst, deviceDigitalGallery, deviceDigitalGalleryAnnc, deviceDigitalGalleryInst, deviceDishWasher, deviceDishWasherAnnc, deviceDishWasherInst, deviceFan, deviceFanAnnc, deviceFanInst, deviceFoodProbe, deviceFoodProbeAnnc, deviceFoodProbeInst, deviceFreezer, deviceFreezerAnnc, deviceFreezerInst, deviceGarbageDisposal, deviceGarbageDisposalAnnc, deviceGarbageDisposalInst, deviceHomeCCTV, deviceHomeCCTVAnnc, deviceHomeCCTVInst, deviceHumidifier, deviceHumidifierAnnc, deviceHumidifierInst, deviceKettle, deviceKettleAnnc, deviceKettleInst, deviceMicrogeneration, deviceMicrogenerationAnnc, deviceMicrogenerationInst, deviceOven, deviceOvenAnnc, deviceOvenInst, deviceRefrigerator, deviceRefrigeratorAnnc, deviceRefrigeratorInst, deviceRiceCooker, deviceRiceCookerAnnc, deviceRiceCookerInst, deviceRobotCleaner, deviceRobotCleanerAnnc, deviceRobotCleanerInst, deviceSecurityPanel, deviceSecurityPanelAnnc, deviceSecurityPanelInst, deviceSetTopBox, deviceSetTopBoxAnnc, deviceSetTopBoxInst, deviceSteamCloset, deviceSteamClosetAnnc, deviceSteamClosetInst, deviceStorageBattery, deviceStorageBatteryAnnc, deviceStorageBatteryInst, deviceTelevision, deviceTelevisionAnnc, deviceTelevisionInst, deviceWaterHeater, deviceWaterHeaterAnnc, deviceWaterHeaterInst, deviceWaterPurifier, deviceWaterPurifierAnnc, deviceWaterPurifierInst, deviceWindowShade, deviceWindowShadeAnnc, deviceWindowShadeInst, flexNode, flexNodeAnnc, flexNodeInst, deviceHandheldPTTTerminal, deviceHandheldPTTTerminalAnnc, deviceHandheldPTTTerminalInst, deviceTrainborneTerminal, deviceTrainborneTerminalAnnc, deviceTrainborneTerminalInst, deviceCardRechargingMachine, deviceCardRechargingMachineAnnc, deviceCardRechargingMachineInst, deviceSmartGate, deviceSmartGateAnnc, deviceSmartGateInst, deviceSmartScreenDoor, deviceSmartScreenDoorAnnc, deviceSmartScreenDoorInst, deviceElectricVehicleCharger, deviceElectricVehicleChargerAnnc, deviceElectricVehicleChargerInst, devicePWSCenter, devicePWSCenterAnnc, devicePWSCenterInst, devicePWSEquipment, devicePWSEquipmentAnnc, devicePWSEquipmentInst | flNLk |
| flowInterval | waterMeterSetting, waterMeterSettingAnnc, waterMeterSettingInst | floIl |
| foaming | milkFoaming | foamg |
| foamingStrength | foaming, foamingAnnc, foamingInst | foaSh |
| forcedUnmounts | dmStorage, dmStorageAnnc, dmStorageInst | forUs |
| format |  | formt |
| frequency | energyConsumption, energyConsumptionAnnc, energyConsumptionInst | freqy |
| friendlyLocation | location, locationAnnc, locationInst, localization, localizationAnnc, localizationInst | friLn |
| friendlyName | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst, localization, localizationAnnc, localizationInst | friNe |
| ftu | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | ftu |
| galleryMode |  | galMe |
| gasChargingControl |  | gaCCl |
| gasMeterAlarm |  | gaMAm |
| gasMeterReportInfo |  | gMRIo |
| generationSource | energyGeneration, energyGenerationAnnc, energyGenerationInst | genSe |
| geoJSON | location, locationAnnc, locationInst | geoJN |
| geoLocation |  | geoLn |
| glucometer |  | glucr |
| grainsRemaining | grinder, grinderAnnc, grinderInst | graRg |
| green | colour, colourAnnc, colourInst | green |
| grinder |  | grinr |
| hangup |  | hangp |
| hash | binaryObject, binaryObjectAnnc, binaryObjectInst | hash |
| hba1c | glucometer, glucometerAnnc, glucometerInst | hba1c |
| heading | geoLocation, geoLocationAnnc, geoLocationInst, headingSensor, headingSensorAnnc, headingSensorInst | headg |
| headingAccuracy | geoLocation, geoLocationAnnc, geoLocationInst, headingSensor, headingSensorAnnc, headingSensorInst | heaAy |
| headingSensor | crossingSensor | heaSr |
| heatingLevel | heatingZone, heatingZoneAnnc, heatingZoneInst | heaLl |
| heatingZone |  | heaZe |
| height | heightAnnc, heightInst, rainGauge, rainGaugeAnnc, rainGaugeInst | heigt |
| hg | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | hg |
| highFlowAlarm | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | hiFAm |
| highFlowAlarmThreshold | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | hFATd |
| highFlowDuration | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | hiFDn |
| highMagneticAlarm | magneticSensorParameters, magneticSensorParametersAnnc, magneticSensorParametersInst | hiMAm |
| highPressureAlarm | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | hiPAm |
| highPressureAlarmThreshold | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | hPATd |
| highTemperatureAlarm | temperatureAlarm, temperatureAlarmAnnc, temperatureAlarmInst, waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | hiTAm |
| highTemperatureAlarmThreshold | temperatureAlarm, temperatureAlarmAnnc, temperatureAlarmInst, waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | hTATd |
| highTemperatureInnerAlarmThreshold | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | hTIAT |
| historyStepCounts | cowActivityMonitor, cowActivityMonitorAnnc, cowActivityMonitorInst | hiSCs |
| horizontalAccuracy | geoLocation, geoLocationAnnc, geoLocationInst | horAy |
| horizontalDirection | airFlow, airFlowAnnc, airFlowInst | horDn |
| hostedAELinks | flexNode, flexNodeAnnc, flexNodeInst | hAELs |
| hostedServiceLinks | flexNode, flexNodeAnnc, flexNodeInst | hoSLs |
| hotWaterSupply |  | hoWSy |
| humidity | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | humiy |
| hwVersion | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst | hweVn |
| identifier | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | idenr |
| impactDirectionHorizontal | impactSensor, impactSensorAnnc, impactSensorInst | imDHl |
| impactDirectionVertical | impactSensor, impactSensorAnnc, impactSensorInst | imDVl |
| impactLevel | impactSensor, impactSensorAnnc, impactSensorInst | impLl |
| impactSensor |  | impSr |
| impactStatus | impactSensor, impactSensorAnnc, impactSensorInst | impSs |
| impedance | bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst | impee |
| impinorganicSaltMassedance | bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst | imSMe |
| impulseFault | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | impFt |
| incrementNumberValue |  | inNVe |
| infraredSensor |  | infSr |
| initialMagnetic | magneticSensorParameters, magneticSensorParametersAnnc, magneticSensorParametersInst | iniMc |
| innerErrorAlarm | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | inEAm |
| innerHighInternalTemperatureAlarm | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | iHITA |
| innerTemperatureSensorFault | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | iTSFt |
| install |  | instl |
| intensiveReportInterval | waterMeterSetting, waterMeterSettingAnnc, waterMeterSettingInst | inRIl |
| intensiveReportStartTime | waterMeterSetting, waterMeterSettingAnnc, waterMeterSettingInst | iRSTe |
| intensiveSampleInterval | waterMeterSetting, waterMeterSettingAnnc, waterMeterSettingInst | inSIl |
| intervalFlow | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | intFw |
| jobModes | airConJobMode, airConJobModeAnnc, airConJobModeInst, airPurifierJobMode, airPurifierJobModeAnnc, airPurifierJobModeInst, clothesDryerJobMode, clothesDryerJobModeAnnc, clothesDryerJobModeInst, clothesWasherDryerJobMode, clothesWasherDryerJobModeAnnc, clothesWasherDryerJobModeInst, clothesWasherJobMode, clothesWasherJobModeAnnc, clothesWasherJobModeInst, cookerHoodJobMode, cookerHoodJobModeAnnc, cookerHoodJobModeInst, dehumidifierJobMode, dehumidifierJobModeAnnc, dehumidifierJobModeInst, dishWasherJobMode, dishWasherJobModeAnnc, dishWasherJobModeInst, robotCleanerJobMode, robotCleanerJobModeAnnc, robotCleanerJobModeInst, steamClosetJobMode, steamClosetJobModeAnnc, steamClosetJobModeInst | jobMs |
| jobStates | runState, runStateAnnc, runStateInst | jobSs |
| kcal | bioElectricalImpedanceAnalysis, bioElectricalImpedanceAnalysisAnnc, bioElectricalImpedanceAnalysisInst | kcal |
| keepWarm |  | keeWm |
| keyNumber | keypad, keypadAnnc, keypadInst | keyNr |
| keypad |  | keypd |
| kmno4 | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | kmno4 |
| lampTechnology | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | lamTy |
| largeFlowAlarm | gasMeterAlarm, gasMeterAlarmAnnc, gasMeterAlarmInst | laFAm |
| latitude | geoLocation, geoLocationAnnc, geoLocationInst | latie |
| leakageAlarm | gasMeterAlarm, gasMeterAlarmAnnc, gasMeterAlarmInst | leaAm |
| level | battery, batteryAnnc, batteryInst | lvl |
| light | alarmSpeaker, alarmSpeakerAnnc, alarmSpeakerInst | light |
| lightActivePower | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | liAPr |
| lightApparentPower | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | liAP0 |
| lightCount | slcParameterSetting, slcParameterSettingAnnc, slcParameterSettingInst | ligCt |
| lightCurrent | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | ligC0 |
| lightDimmingValue | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | liDVe |
| lightPolarizationAxis | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | liPAs |
| lightPowerFactor | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | liPFr |
| lightReactivePower | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | liRPr |
| lightVoltage | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | ligVe |
| liquidLevel | liquidLevelAnnc, liquidLevelInst, milkQuantity | liqLl |
| liquidRemaining | liquidRemainingAnnc, liquidRemainingInst, waterStatus, waterLevel | liqRg |
| locale | localization, localizationAnnc, localizationInst | locae |
| localization |  | loca0 |
| location |  | locan |
| lock | doorlock, doorLock, lockAnnc, lockInst, controlPanelLock | lock |
| lockedDownAlarm | gasMeterAlarm, gasMeterAlarmAnnc, gasMeterAlarmInst | loDAm |
| loginName | credentials, credentialsAnnc, credentialsInst | logNe |
| longitude | geoLocation, geoLocationAnnc, geoLocationInst | longe |
| loudness | acousticSensor, acousticSensorAnnc, acousticSensorInst | louds |
| lowBattery | battery, batteryAnnc, batteryInst | lowBy |
| lowCreditAlarm | gasMeterAlarm, gasMeterAlarmAnnc, gasMeterAlarmInst | loCAm |
| lowestFlowRate | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | loFRe |
| lowestFlowRateTime | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | lFRTe |
| lowestReverseFlowRate | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | lRFRe |
| lowestReverseFlowRateTime | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | lRFRT |
| lowFlowAlarm | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | loFAm |
| lowFlowAlarmThreshold | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | lFATd |
| lowFlowDuration | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | loFDn |
| lowGasAlarm | gasMeterAlarm, gasMeterAlarmAnnc, gasMeterAlarmInst | loGAm |
| lowPressureAlarm | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | loPAm |
| lowPressureAlarmThreshold | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | lPATd |
| lowTemperatureAlarm | temperatureAlarm, temperatureAlarmAnnc, temperatureAlarmInst, waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | loTAm |
| lowTemperatureAlarmThreshold | temperatureAlarm, temperatureAlarmAnnc, temperatureAlarmInst, waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | lTATd |
| lowVoltage | smokeSensor, smokeSensorAnnc, smokeSensorInst | lowVe |
| lqi | signalStrength, signalStrengthAnnc, signalStrengthInst | lqi |
| machineStates | runState, runStateAnnc, runStateInst | macSs |
| magneticDisturb | gasMeterAlarm, gasMeterAlarmAnnc, gasMeterAlarmInst | magDb |
| magneticInterference | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | magIe |
| magneticSensitivityLevel | magneticSensorParameters, magneticSensorParametersAnnc, magneticSensorParametersInst | maSLl |
| magneticSensorParameters |  | maSPs |
| manufacturer | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst | manur |
| manufacturerDetailsLink | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst | maDLk |
| manufacturingDate | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst | manDe |
| maxHeatingLevel | heatingZone, heatingZoneAnnc, heatingZoneInst | maHLl |
| maxLength | textMessage, textMessageAnnc, textMessageInst | maxLh |
| maxLevel | openLevel, openLevelAnnc, openLevelInst | maxLl |
| maxPressureThreshold | barometer, barometerAnnc, barometerInst | maPTd |
| maxSizeX | threeDScanner, threeDScannerAnnc, threeDScannerInst | maxSX |
| maxSizeY | threeDScanner, threeDScannerAnnc, threeDScannerInst | maxSY |
| maxSizeZ | threeDScanner, threeDScannerAnnc, threeDScannerInst | maxSZ |
| maxSpeed | airFlow, airFlowAnnc, airFlowInst | maxSd |
| maxValue | audioVolume, audioVolumeAnnc, audioVolumeInst, numberValue, numberValueAnnc, numberValueInst, ozoneMeter, ozoneMeterAnnc, ozoneMeterInst, temperature, temperatureAnnc, temperatureInst | maxVe |
| meanPressure | sphygmomanometer, sphygmomanometerAnnc, sphygmomanometerInst | meaPe |
| measuringScope | energyConsumption, energyConsumptionAnnc, energyConsumptionInst | meaSe |
| mediaID | mediaSelect, mediaSelectAnnc, mediaSelectInst | medID |
| mediaName | mediaSelect, mediaSelectAnnc, mediaSelectInst | medNe |
| mediaSelect | mediaInput, pictureInput | medSt |
| mediaType | mediaSelect, mediaSelectAnnc, mediaSelectInst | medTe |
| memorySize | threeDPrinter, threeDPrinterAnnc, threeDPrinterInst | memSe |
| messageEncoding | textMessage, textMessageAnnc, textMessageInst | mesEg |
| metadata | features, featuresAnnc, featuresInst | metaa |
| minimumCommunicationLatency | connectivity, connectivityAnnc, connectivityInst | miCLy |
| minLength | textMessage, textMessageAnnc, textMessageInst | minLh |
| minLevel | openLevel, openLevelAnnc, openLevelInst | minLl |
| minPressureThreshold | barometer, barometerAnnc, barometerInst | miPTd |
| minSpeed | airFlow, airFlowAnnc, airFlowInst | minSd |
| minValue | numberValue, numberValueAnnc, numberValueInst, temperature, temperatureAnnc, temperatureInst | minVe |
| modality | pulsemeter, pulsemeterAnnc, pulsemeterInst | moday |
| model | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst | model |
| monitoringEnabled | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | monEd |
| motionSensor |  | motSr |
| mountingPoint | dmStorage, dmStorageAnnc, dmStorageInst | mouPt |
| mountOptions | dmStorage, dmStorageAnnc, dmStorageInst | mouOs |
| mounts | dmStorage, dmStorageAnnc, dmStorageInst | mouns |
| msgType | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | msgTe |
| multiFirmware | dmFirmware, dmFirmwareAnnc, dmFirmwareInst | mulFe |
| multiplyingFactors | energyConsumption, energyConsumptionAnnc, energyConsumptionInst, energyGeneration, energyGenerationAnnc, energyGenerationInst | mulFs |
| muscle | bioElectricalImpedanceAnalysis, bioElectricalImpedanceAnalysisAnnc, bioElectricalImpedanceAnalysisInst | musce |
| muscleMass | bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst | musMs |
| mute |  | mute |
| muteAudioVolume |  | muAVe |
| muteEnabled | audioVolume, audioVolumeAnnc, audioVolumeInst | mutEd |
| name | dmSoftware, dmSoftwareAnnc, dmSoftwareInst, dmPackage, dmPackageAnnc, dmPackageInst, dmCapability, dmCapabilityAnnc, dmCapabilityInst, dmStorage, dmStorageAnnc, dmStorageInst, deployPackage, deployPackageAnnc, deployPackageInst | name |
| needsReplacement | filterInfo, filterInfoAnnc, filterInfoInst | neeRt |
| negativeCumulativeFlow | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | neCFw |
| network | threeDPrinter, threeDPrinterAnnc, threeDPrinterInst | netwk |
| nextTrack |  | nexTk |
| nh3nh4 | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | nh3n4 |
| no2 | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | no2 |
| no3n | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | no3n |
| nodeID | flexNode, flexNodeAnnc, flexNodeInst | nodID |
| nodeLink | device3DPrinter, device3DPrinterAnnc, device3DPrinterInst, deviceAirQualityMonitor, deviceAirQualityMonitorAnnc, deviceAirQualityMonitorInst, deviceAudioReceiver, deviceAudioReceiverAnnc, deviceAudioReceiverInst, deviceCamera, deviceCameraAnnc, deviceCameraInst, deviceDoor, deviceDoorAnnc, deviceDoorInst, deviceDoorLock, deviceDoorLockAnnc, deviceDoorLockInst, deviceGenericSensor, deviceGenericSensorAnnc, deviceGenericSensorInst, deviceLight, deviceLightAnnc, deviceLightInst, deviceMultiFunctionPrinter, deviceMultiFunctionPrinterAnnc, deviceMultiFunctionPrinterInst, devicePrinter, devicePrinterAnnc, devicePrinterInst, deviceScanner, deviceScannerAnnc, deviceScannerInst, deviceServiceButton, deviceServiceButtonAnnc, deviceServiceButtonInst, deviceSmartPlug, deviceSmartPlugAnnc, deviceSmartPlugInst, deviceSwitch, deviceSwitchAnnc, deviceSwitchInst, deviceThermometer, deviceThermometerAnnc, deviceThermometerInst, deviceThermostat, deviceThermostatAnnc, deviceThermostatInst, deviceWaterValve, deviceWaterValveAnnc, deviceWaterValveInst, device3DDisplay, device3DDisplayAnnc, device3DDisplayInst, device3DScanner, device3DScannerAnnc, device3DScannerInst, deviceCowActivityMonitor, deviceCowActivityMonitorAnnc, deviceCowActivityMonitorInst, deviceOutdoorLamp, deviceOutdoorLampAnnc, deviceOutdoorLampInst, deviceMagneticParkingMonitor, deviceMagneticParkingMonitorAnnc, deviceMagneticParkingMonitorInst, deviceSmartElectricMeter, deviceSmartElectricMeterAnnc, deviceSmartElectricMeterInst, deviceSmartGasMeter, deviceSmartGasMeterAnnc, deviceSmartGasMeterInst, deviceSmartWaterMeter, deviceSmartWaterMeterAnnc, deviceSmartWaterMeterInst, deviceStreetLightController, deviceStreetLightControllerAnnc, deviceStreetLightControllerInst, deviceWaterQualityMonitor, deviceWaterQualityMonitorAnnc, deviceWaterQualityMonitorInst, deviceWeatherStation, deviceWeatherStationAnnc, deviceWeatherStationInst, deviceBloodPressureMonitor, deviceBloodPressureMonitorAnnc, deviceBloodPressureMonitorInst, deviceGlucosemeter, deviceGlucosemeterAnnc, deviceGlucosemeterInst, deviceHeartRateMonitor, deviceHeartRateMonitorAnnc, deviceHeartRateMonitorInst, devicePulseOximeter, devicePulseOximeterAnnc, devicePulseOximeterInst, deviceWeightScaleAndBodyCompositionAnalyser, deviceWeightScaleAndBodyCompositionAnalyserAnnc, deviceWeightScaleAndBodyCompositionAnalyserInst, deviceAirConditioner, deviceAirConditionerAnnc, deviceAirConditionerInst, deviceAirPurifier, deviceAirPurifierAnnc, deviceAirPurifierInst, deviceBottleWarmer, deviceBottleWarmerAnnc, deviceBottleWarmerInst, deviceClothesDryer, deviceClothesDryerAnnc, deviceClothesDryerInst, deviceClothesWasher, deviceClothesWasherAnnc, deviceClothesWasherInst, deviceClothesWasherDryer, deviceClothesWasherDryerAnnc, deviceClothesWasherDryerInst, deviceCoffeeMachine, deviceCoffeeMachineAnnc, deviceCoffeeMachineInst, deviceCookerHood, deviceCookerHoodAnnc, deviceCookerHoodInst, deviceCooktop, deviceCooktopAnnc, deviceCooktopInst, deviceDehumidifier, deviceDehumidifierAnnc, deviceDehumidifierInst, deviceDigitalGallery, deviceDigitalGalleryAnnc, deviceDigitalGalleryInst, deviceDishWasher, deviceDishWasherAnnc, deviceDishWasherInst, deviceFan, deviceFanAnnc, deviceFanInst, deviceFoodProbe, deviceFoodProbeAnnc, deviceFoodProbeInst, deviceFreezer, deviceFreezerAnnc, deviceFreezerInst, deviceGarbageDisposal, deviceGarbageDisposalAnnc, deviceGarbageDisposalInst, deviceHomeCCTV, deviceHomeCCTVAnnc, deviceHomeCCTVInst, deviceHumidifier, deviceHumidifierAnnc, deviceHumidifierInst, deviceKettle, deviceKettleAnnc, deviceKettleInst, deviceMicrogeneration, deviceMicrogenerationAnnc, deviceMicrogenerationInst, deviceOven, deviceOvenAnnc, deviceOvenInst, deviceRefrigerator, deviceRefrigeratorAnnc, deviceRefrigeratorInst, deviceRiceCooker, deviceRiceCookerAnnc, deviceRiceCookerInst, deviceRobotCleaner, deviceRobotCleanerAnnc, deviceRobotCleanerInst, deviceSecurityPanel, deviceSecurityPanelAnnc, deviceSecurityPanelInst, deviceSetTopBox, deviceSetTopBoxAnnc, deviceSetTopBoxInst, deviceSteamCloset, deviceSteamClosetAnnc, deviceSteamClosetInst, deviceStorageBattery, deviceStorageBatteryAnnc, deviceStorageBatteryInst, deviceTelevision, deviceTelevisionAnnc, deviceTelevisionInst, deviceWaterHeater, deviceWaterHeaterAnnc, deviceWaterHeaterInst, deviceWaterPurifier, deviceWaterPurifierAnnc, deviceWaterPurifierInst, deviceWindowShade, deviceWindowShadeAnnc, deviceWindowShadeInst, flexNode, flexNodeAnnc, flexNodeInst, deviceHandheldPTTTerminal, deviceHandheldPTTTerminalAnnc, deviceHandheldPTTTerminalInst, deviceTrainborneTerminal, deviceTrainborneTerminalAnnc, deviceTrainborneTerminalInst, deviceCardRechargingMachine, deviceCardRechargingMachineAnnc, deviceCardRechargingMachineInst, deviceSmartGate, deviceSmartGateAnnc, deviceSmartGateInst, deviceSmartScreenDoor, deviceSmartScreenDoorAnnc, deviceSmartScreenDoorInst, deviceElectricVehicleCharger, deviceElectricVehicleChargerAnnc, deviceElectricVehicleChargerInst, devicePWSCenter, devicePWSCenterAnnc, devicePWSCenterInst, devicePWSEquipment, devicePWSEquipmentAnnc, devicePWSEquipmentInst | nodLk |
| noise | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | noise |
| numberValue | numberValueAnnc, numberValueInst, dimmingLevel | numVe |
| o3 | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | o3 |
| object | binaryObject, binaryObjectAnnc, binaryObjectInst | objet |
| objectType | binaryObject, binaryObjectAnnc, binaryObjectInst | objTe |
| odor | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | odor |
| oil | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | oil |
| onlineStatus | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | onlSs |
| onset | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | onset |
| open |  | open |
| openAlarm | doorStatus, doorStatusAnnc, doorStatusInst | opeAm |
| openDuration | doorStatus, doorStatusAnnc, doorStatusInst | opeDn |
| openLevel | openLevelAnnc, openLevelInst | opeLl |
| operationMode | airConOperationMode, airPurifierOperationMode, clothesDryerOperationMode, clothesWasherOperationMode, clothesWasherDryerOperationMode, dehumidifierOperationMode, robotCleanerOperationMode, steamClosetOperationMode | opeMe |
| optoutStatus | settings, settingsAnnc, settingsInst | optSs |
| origin |  | orign |
| originID | origin, originAnnc, originInst | oriID |
| osVersion | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst | oseVn |
| overCurrentAlarm | slcAlarm, slcAlarmAnnc, slcAlarmInst | ovCAm |
| overCurrentDuration | slcAlarm, slcAlarmAnnc, slcAlarmInst | ovCDn |
| overcurrentSensor |  | oveSr |
| overcurrentStatus | overcurrentSensor, overcurrentSensorAnnc, overcurrentSensorInst | oveSs |
| overCurrentThreshold | slcAlarm, slcAlarmAnnc, slcAlarmInst | ovCTd |
| overVoltageAlarm | slcAlarm, slcAlarmAnnc, slcAlarmInst | ovVAm |
| overVoltageDuration | slcAlarm, slcAlarmAnnc, slcAlarmInst | ovVDn |
| overVoltagePercent | slcAlarm, slcAlarmAnnc, slcAlarmInst | ovVPt |
| overVoltageThreshold | slcAlarm, slcAlarmAnnc, slcAlarmInst | ovVTd |
| oximeter |  | oximr |
| oxygenSaturation | oximeter, oximeterAnnc, oximeterInst | oxySn |
| ozoneMeter |  | ozoMr |
| ozoneStatus | ozoneMeter, ozoneMeterAnnc, ozoneMeterInst | ozoSs |
| ozoneValueMG | ozoneMeter, ozoneMeterAnnc, ozoneMeterInst | ozVMG |
| ozoneValuePPM | ozoneMeter, ozoneMeterAnnc, ozoneMeterInst, parkingStatus, parkingStatusAnnc, parkingStatusInst | oVPPM |
| p25 | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | p25 |
| parkingStatus |  | parSs |
| password | credentials, credentialsAnnc, credentialsInst | pwd |
| payload | writeIO, writeIOAnnc, writeIOInst | payld |
| pb | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | pb |
| pci | connectivity, connectivityAnnc, connectivityInst | pci |
| peakFlowRate | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | peFRe |
| peakFlowRateTime | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | pFRTe |
| peakReverseFlowRate | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | pRFRe |
| peakReverseFlowRateTime | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | pRFRT |
| period | periodicalReportConfig, periodicalReportConfigAnnc, periodicalReportConfigInst | perid |
| periodicalReportConfig |  | peRCg |
| ph | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | ph |
| phoneCall |  | phoCl |
| playerControl |  | plaCl |
| pm1 | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | pm1 |
| pm10 | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | pm10 |
| positionX | touchScreen, touchScreenAnnc, touchScreenInst | posiX |
| positionY | touchScreen, touchScreenAnnc, touchScreenInst | posiY |
| postalAddress | location, locationAnnc, locationInst | posAs |
| power | energyConsumption, energyConsumptionAnnc, energyConsumptionInst | power |
| powerGenerationData | energyGeneration, energyGenerationAnnc, energyGenerationInst | poGDa |
| powerOn | smokeSensor, smokeSensorAnnc, smokeSensorInst | powOn |
| powerSave |  | powS0 |
| powerSaveEnabled | powerSave, powerSaveAnnc, powerSaveInst | poSEd |
| powerState | binarySwitch, binarySwitchAnnc, binarySwitchInst | powSe |
| powerStatus | dmAgent, dmAgentAnnc, dmAgentInst | powSs |
| precision | features, featuresAnnc, featuresInst | precn |
| prePaidCardReader | ticketReader | pPCRr |
| presence | dmStorage, dmStorageAnnc, dmStorageInst | prese |
| presentationURL | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst | prURL |
| pressureSensorFault | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | prSFt |
| previousChannel | televisionChannel, televisionChannelAnnc, televisionChannelInst | preCl |
| previousTrack |  | preTk |
| preWash | clothesWasherJobModeOption, clothesWasherJobModeOptionAnnc, clothesWasherJobModeOptionInst | preWh |
| primaryName | dmFirmware, dmFirmwareAnnc, dmFirmwareInst | priNe |
| primaryState | dmFirmware, dmFirmwareAnnc, dmFirmwareInst | priSe |
| primaryUrl | dmFirmware, dmFirmwareAnnc, dmFirmwareInst | priUl |
| primaryVersion | dmFirmware, dmFirmwareAnnc, dmFirmwareInst | priVn |
| printingState | printQueue, printQueueAnnc, printQueueInst | priS0 |
| printQueue |  | priQe |
| printSizeX | threeDPrinter, threeDPrinterAnnc, threeDPrinterInst | priSX |
| printSizeY | threeDPrinter, threeDPrinterAnnc, threeDPrinterInst | priSY |
| printSizeZ | threeDPrinter, threeDPrinterAnnc, threeDPrinterInst | priSZ |
| printType | threeDPrinter, threeDPrinterAnnc, threeDPrinterInst | priTe |
| progressPercentage | runState, runStateAnnc, runStateInst | proPe |
| proteinMass | bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst | proMs |
| pulsemeter |  | pulsr |
| pulseRate | pulsemeter, pulsemeterAnnc, pulsemeterInst | pulRe |
| pushButton | pttButton, emergencyButton | pusBn |
| pushed | pushButton, pushButtonAnnc, pushButtonInst, touchScreen, touchScreenAnnc, touchScreenInst | pushd |
| rainGauge |  | raiGe |
| ramAvailable | dmAgent, dmAgentAnnc, dmAgentInst | ramAe |
| ramTotal | dmAgent, dmAgentAnnc, dmAgentInst | ramTl |
| rapidCool | refrigeration, refrigerationAnnc, refrigerationInst | rapCl |
| rapidFreeze | refrigeration, refrigerationAnnc, refrigerationInst | rapFe |
| readIO |  | reaIO |
| readSpeed | dmStorage, dmStorageAnnc, dmStorageInst | reaSd |
| readStatus | prePaidCardReader, prePaidCardReaderAnnc, prePaidCardReaderInst | reaSs |
| reboot |  | rebot |
| rebootType | reboot, rebootAnnc, rebootInst | rebTe |
| rechargeable | battery, batteryAnnc, batteryInst | reche |
| rechargeCredit | gasChargingControl, gasChargingControlAnnc, gasChargingControlInst | recCt |
| rechargeGas | gasChargingControl, gasChargingControlAnnc, gasChargingControlInst | recGs |
| recipientID | phoneCall, phoneCallAnnc, phoneCallInst | recID |
| recorder |  | recor |
| red | colour, colourAnnc, colourInst | red |
| references | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | refes |
| referenceTimer | timer, timerAnnc, timerInst | refTr |
| refrigeration |  | refrn |
| relativeHumidity | relativeHumidityAnnc, relativeHumidityInst | relHy |
| reliability | features, featuresAnnc, featuresInst | reliy |
| remoteControlEnable |  | reCEe |
| remoteControlEnabled | remoteControlEnable, remoteControlEnableAnnc, remoteControlEnableInst | reCEd |
| repetitionCount | disseminator, disseminatorAnnc, disseminatorInst | repCt |
| repetitionPeriod | disseminator, disseminatorAnnc, disseminatorInst | repPd |
| reset |  | reset |
| resetNumberValue |  | reNVe |
| resetTextMessage |  | reTMe |
| resistance | bioElectricalImpedanceAnalysis, bioElectricalImpedanceAnalysisAnnc, bioElectricalImpedanceAnalysisInst | resie |
| result | deployPackage, deployPackageAnnc, deployPackageInst, writeIO, writeIOAnnc, writeIOInst, updateFirmware, updateFirmwareAnnc, updateFirmwareInst, disable, disableAnnc, disableInst, enable, enableAnnc, enableInst, readIO, readIOAnnc, readIOInst, cancel, cancelAnnc, cancelInst | resut |
| retrieveLog |  | retLg |
| retryInterval | periodicalReportConfig, periodicalReportConfigAnnc, periodicalReportConfigInst | retIl |
| retryTimes | periodicalReportConfig, periodicalReportConfigAnnc, periodicalReportConfigInst | retTs |
| reverseFlowAlarm | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | reFAm |
| reverseFlowAlarmThreshold | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | rFATd |
| reverseFlowDuration | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | reFDn |
| reverseFlowInterval | waterMeterSetting, waterMeterSettingAnnc, waterMeterSettingInst | reFIl |
| reverseIntervalFlow | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | reIFw |
| robotCleanerJobMode |  | rCJMe |
| room | location, locationAnnc, locationInst | room |
| roundingEnergyConsumption | energyConsumption, energyConsumptionAnnc, energyConsumptionInst | roECn |
| roundingEnergyGeneration | energyGeneration, energyGenerationAnnc, energyGenerationInst | roEGn |
| rr | pulsemeter, pulsemeterAnnc, pulsemeterInst | r0 |
| rsrp | connectivity, connectivityAnnc, connectivityInst | rsrp |
| rsrq | connectivity, connectivityAnnc, connectivityInst | rsrq |
| rssi | connectivity, connectivityAnnc, connectivityInst, signalStrength, signalStrengthAnnc, signalStrengthInst | rssi |
| runningTime | timer, timerAnnc, timerInst | runTe |
| runState | printerRunState, machineState, threeDScanState, gateState | runSe |
| saveAudioVolume | audioVolume, audioVolumeAnnc, audioVolumeInst | saAVe |
| scanStatus | cardScanner, cardScannerAnnc, cardScannerInst | scaSs |
| sdp | sessionDescription, sessionDescriptionAnnc, sessionDescriptionInst | sdp |
| secondaryName | dmFirmware, dmFirmwareAnnc, dmFirmwareInst | secNe |
| secondaryState | dmFirmware, dmFirmwareAnnc, dmFirmwareInst | secSe |
| secondaryUrl | dmFirmware, dmFirmwareAnnc, dmFirmwareInst | secUl |
| secondaryVersion | dmFirmware, dmFirmwareAnnc, dmFirmwareInst | secVn |
| securityMode |  | secMe |
| securityModes | securityMode, securityModeAnnc, securityModeInst | secMs |
| sender | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | sendr |
| sensitivity | motionSensor, motionSensorAnnc, motionSensorInst | sensy |
| sensorFault | smokeSensor, smokeSensorAnnc, smokeSensorInst | senFt |
| sent | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | sent |
| serialNumber | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst | serNr |
| sessionDescription |  | sesDn |
| settings |  | setts |
| severity | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | sevey |
| signal | signalPanel, signalPanelAnnc, signalPanelInst | signl |
| signalECL | connectivity, connectivityAnnc, connectivityInst | siECL |
| signalPanel | directionPanel | sigPl |
| signalStrength |  | sigSh |
| significantDigits | energyConsumption, energyConsumptionAnnc, energyConsumptionInst, energyGeneration, energyGenerationAnnc, energyGenerationInst | sigDs |
| silentTime | motionSensor, motionSensorAnnc, motionSensorInst | silTe |
| singleCountAlarm | gasMeterAlarm, gasMeterAlarmAnnc, gasMeterAlarmInst | siCAm |
| sinr | connectivity, connectivityAnnc, connectivityInst | sinr |
| size | binaryObject, binaryObjectAnnc, binaryObjectInst, features, featuresAnnc, featuresInst | size |
| slcAlarm |  | slcAm |
| slcParameterSetting |  | slPSg |
| slcReportInfo |  | slRIo |
| sleepDuration | dmAreaNwkDeviceInfo, dmAreaNwkDeviceInfoAnnc, dmAreaNwkDeviceInfoInst | sleDn |
| sleepInterval | dmAreaNwkDeviceInfo, dmAreaNwkDeviceInfoAnnc, dmAreaNwkDeviceInfoInst | sleIl |
| smokeSensor |  | smoSr |
| smokeThreshold | smokeSensor, smokeSensorAnnc, smokeSensorInst | smoT0 |
| so2 | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | so2 |
| softLeanMass | bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst | soLMs |
| softwares | dmPackage, dmPackageAnnc, dmPackageInst | softs |
| soilLevel | clothesWasherJobModeOption, clothesWasherJobModeOptionAnnc, clothesWasherJobModeOptionInst | soiLl |
| somatotype | bodyCompositionAnalyser, bodyCompositionAnalyserAnnc, bodyCompositionAnalyserInst | somae |
| speed | airFlow, airFlowAnnc, airFlowInst, anemometer, anemometerAnnc, anemometerInst | speed |
| speedFactor | playerControl, playerControlAnnc, playerControlInst | speFr |
| speedWash | clothesWasherJobModeOption, clothesWasherJobModeOptionAnnc, clothesWasherJobModeOptionInst | speWh |
| sphygmomanometer |  | sphyr |
| spinLevel |  | spiLl |
| spinLevelStrength | spinLevel, spinLevelAnnc, spinLevelInst | spLSh |
| spinSpeed | clothesWasherJobModeOption, clothesWasherJobModeOptionAnnc, clothesWasherJobModeOptionInst | spiSd |
| standardreferenceVoltage | slcAlarm, slcAlarmAnnc, slcAlarmInst | staVe |
| start | retrieveLog, retrieveLogAnnc, retrieveLogInst | start |
| start3Dprint |  | staDt |
| startPause | operationMode, operationModeAnnc, operationModeInst | staPe |
| state | dmAgent, dmAgentAnnc, dmAgentInst, dmSoftware, dmSoftwareAnnc, dmSoftwareInst, dmPackage, dmPackageAnnc, dmPackageInst | state |
| status | boiler, boilerAnnc, boilerInst, electricVehicleConnector, electricVehicleConnectorAnnc, electricVehicleConnectorInst, faultDetection, faultDetectionAnnc, faultDetectionInst, mediaSelect, mediaSelectAnnc, mediaSelectInst, dmEventLog, dmEventLogAnnc, dmEventLogInst, dmAreaNwkDeviceInfo, dmAreaNwkDeviceInfoAnnc, dmAreaNwkDeviceInfoInst, dmStorage, dmStorageAnnc, dmStorageInst, disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | sus |
| steamClosetJobMode |  | sCJMe |
| steamTreat | clothesWasherJobModeOption, clothesWasherJobModeOptionAnnc, clothesWasherJobModeOptionInst | steTt |
| step | numberValue, numberValueAnnc, numberValueInst | step |
| stepsPerPeriod | cowActivityMonitor, cowActivityMonitorAnnc, cowActivityMonitorInst | stPPd |
| stepValue | audioVolume, audioVolumeAnnc, audioVolumeInst, openLevel, openLevelAnnc, openLevelInst, temperature, temperatureAnnc, temperatureInst | steVe |
| stop3Dprint |  | stoDt |
| storageAvailable | dmAgent, dmAgentAnnc, dmAgentInst | stoAe |
| storageFault | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | stoFt |
| storageTotal | dmAgent, dmAgentAnnc, dmAgentInst | stoTl |
| strength | brewing, brewingAnnc, brewingInst | streh |
| subDeviceCuff |  | suDCf |
| subDevicePowerOutlet |  | sDPOt |
| subModel | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst | subMl |
| sulfide | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | sulfe |
| supportedHorizontalDirection | airFlow, airFlowAnnc, airFlowInst | suHDn |
| supportedMediaSources | mediaSelect, mediaSelectAnnc, mediaSelectInst | suMSs |
| supportedMessageValues | textMessage, textMessageAnnc, textMessageInst | suMVs |
| supportedPlayerModes | playerControl, playerControlAnnc, playerControlInst | suPMs |
| supportedVerticalDirection | airFlow, airFlowAnnc, airFlowInst | suVDn |
| supportURL | dmDeviceInfo, dmDeviceInfoAnnc, dmDeviceInfoInst | suURL |
| surplusCredit | gasChargingControl, gasChargingControlAnnc, gasChargingControlInst | surCt |
| surplusGas | gasChargingControl, gasChargingControlAnnc, gasChargingControlInst | surGs |
| switchStatus | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | swiSs |
| systemTime | dmAgent, dmAgentAnnc, dmAgentInst | sysTe |
| systolicPressure | sphygmomanometer, sphygmomanometerAnnc, sphygmomanometerInst | sysPe |
| tamperAlarm | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | tamAm |
| targetAltitude | geoLocation, geoLocationAnnc, geoLocationInst | tarAe |
| targetDuration | timer, timerAnnc, timerInst | tarDn |
| targetLatitude | geoLocation, geoLocationAnnc, geoLocationInst | tarLe |
| targetLongitude | geoLocation, geoLocationAnnc, geoLocationInst | tarL0 |
| targetTemperature | keepWarm, keepWarmAnnc, keepWarmInst, temperature, temperatureAnnc, temperatureInst | tarTe |
| targetTimeToStart | timer, timerAnnc, timerInst | tTTSt |
| targetTimeToStop | timer, timerAnnc, timerInst | tTTSp |
| telegramMessage | baliseTransmissionModule, baliseTransmissionModuleAnnc, baliseTransmissionModuleInst | telMe |
| televisionChannel | channel | telCl |
| temperature | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst, temperatureAlarm, temperatureAlarmAnnc, temperatureAlarmInst, waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst, outdoorTemperature, frozenTemperature | tempe |
| temperatureAlarm |  | temAm |
| test |  | test |
| textMessage | textMessageAnnc, textMessageInst | texMe |
| threeDDisplay |  | thDDy |
| threeDDisplayResolutionX | threeDDisplay, threeDDisplayAnnc, threeDDisplayInst | tDDRX |
| threeDDisplayResolutionY | threeDDisplay, threeDDisplayAnnc, threeDDisplayInst | tDDRY |
| threeDDisplayType | threeDDisplay, threeDDisplayAnnc, threeDDisplayInst | tDDTe |
| threeDDisplayViewAngle | threeDDisplay, threeDDisplayAnnc, threeDDisplayInst | tDDVA |
| threeDGlasses | threeDDisplay, threeDDisplayAnnc, threeDDisplayInst | thDGs |
| threeDPrinter |  | thDP0 |
| threeDScanner |  | thDSr |
| threeDScannerType | threeDScanner, threeDScannerAnnc, threeDScannerInst | tDSTe |
| threeDScanResolution | threeDScanner, threeDScannerAnnc, threeDScannerInst | tDSRn |
| time | keepWarm, keepWarmAnnc, keepWarmInst | time |
| timePlanStatus | slcParameterSetting, slcParameterSettingAnnc, slcParameterSettingInst | tiPSs |
| timer | crossingBarrier, crossingBarrierAnnc, crossingBarrierInst | timer |
| timeRangeCount | slcParameterSetting, slcParameterSettingAnnc, slcParameterSettingInst | tiRCt |
| timeRangeLightDimmingValue | slcParameterSetting, slcParameterSettingAnnc, slcParameterSettingInst | tRLDV |
| tn | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | tn |
| toggle |  | togge |
| token | credentials, credentialsAnnc, credentialsInst | tk |
| tone | alarmSpeaker, alarmSpeakerAnnc, alarmSpeakerInst | tone |
| totalStorage | dmStorage, dmStorageAnnc, dmStorageInst | totSe |
| totalUseValue | gasMeterReportInfo, gasMeterReportInfoAnnc, gasMeterReportInfoInst | toUVe |
| touchScreen |  | touSn |
| tp | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | tp |
| tsp | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | tsp |
| turbo |  | turbo |
| turboEnabled | turbo, turboAnnc, turboInst | turEd |
| type | dmEventLog, dmEventLogAnnc, dmEventLogInst, dmPackage, dmPackageAnnc, dmPackageInst, dmStorage, dmStorageAnnc, dmStorageInst | type |
| underCurrentAlarm | slcAlarm, slcAlarmAnnc, slcAlarmInst | unCAm |
| underCurrentDuration | slcAlarm, slcAlarmAnnc, slcAlarmInst | unCDn |
| underCurrentThreshold | slcAlarm, slcAlarmAnnc, slcAlarmInst | unCTd |
| underVoltageAlarm | slcAlarm, slcAlarmAnnc, slcAlarmInst | unVAm |
| underVoltageDuration | slcAlarm, slcAlarmAnnc, slcAlarmInst | unVDn |
| underVoltagePercent | slcAlarm, slcAlarmAnnc, slcAlarmInst | unVPt |
| underVoltageThreshold | slcAlarm, slcAlarmAnnc, slcAlarmInst | unVTd |
| uninstall |  | uninl |
| unit | temperature, temperatureAnnc, temperatureInst, temperatureAlarm, temperatureAlarmAnnc, temperatureAlarmInst, weight, weightAnnc, weightInst | unit |
| unmount |  | unmot |
| unmuteAudioVolume |  | unAVe |
| upChannel |  | uphCl |
| update |  | updae |
| updateFirmware |  | updFe |
| updateTime | cowActivityMonitor, cowActivityMonitorAnnc, cowActivityMonitorInst | updTe |
| upVolume |  | upoVe |
| urgency | disseminator, disseminatorAnnc, disseminatorInst, emergencyHandler, emergencyHandlerAnnc, emergencyHandlerInst | urgey |
| urgencyButtonPush | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | urBPh |
| uri | printQueue, printQueueAnnc, printQueueInst, sessionDescription, sessionDescriptionAnnc, sessionDescriptionInst | ur0 |
| url | dmPackage, dmPackageAnnc, dmPackageInst, deployPackage, deployPackageAnnc, deployPackageInst, updateFirmware, updateFirmwareAnnc, updateFirmwareInst, update, updateAnnc, updateInst | url |
| usedTime | filterInfo, filterInfoAnnc, filterInfoInst | useTe |
| useGrinder | grinder, grinderAnnc, grinderInst | useGr |
| uUID | dmStorage, dmStorageAnnc, dmStorageInst | uUID |
| uvSensor |  | uveSr |
| uvStatus | uvSensor, uvSensorAnnc, uvSensorInst | uvtSs |
| uvValue | uvSensor, uvSensorAnnc, uvSensorInst | uvaVe |
| valveStatus | gasMeterReportInfo, gasMeterReportInfoAnnc, gasMeterReportInfoInst | valSs |
| version | dmSoftware, dmSoftwareAnnc, dmSoftwareInst, dmPackage, dmPackageAnnc, dmPackageInst, deployPackage, deployPackageAnnc, deployPackageInst, updateFirmware, updateFirmwareAnnc, updateFirmwareInst, update, updateAnnc, updateInst | versn |
| verticalAccuracy | geoLocation, geoLocationAnnc, geoLocationInst | verAy |
| verticalDirection | airFlow, airFlowAnnc, airFlowInst | verDn |
| vibrationSensorFault | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | viSFt |
| visceraFat | bioElectricalImpedanceAnalysis, bioElectricalImpedanceAnalysisAnnc, bioElectricalImpedanceAnalysisInst | visFt |
| voc | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | voc |
| voltage | energyConsumption, energyConsumptionAnnc, energyConsumptionInst | volte |
| voltageFrequency | slcReportInfo, slcReportInfoAnnc, slcReportInfoInst | volFy |
| volumeValue | audioVolume, audioVolumeAnnc, audioVolumeInst | volVe |
| warningIdentifier | cancel, cancelAnnc, cancelInst | warIr |
| washTemp | clothesWasherJobModeOption, clothesWasherJobModeOptionAnnc, clothesWasherJobModeOptionInst | wasTp |
| water | bioElectricalImpedanceAnalysis, bioElectricalImpedanceAnalysisAnnc, bioElectricalImpedanceAnalysisInst | water |
| waterFilterInfo | waterfilter | waFIo |
| waterFilterType |  | waFTe |
| waterFlow |  | watFw |
| waterFlowStrength | waterFlow, waterFlowAnnc, waterFlowInst | waFSh |
| waterIntervalPressure | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | waIPe |
| waterIntervalTemperature | waterMeterReportInfo, waterMeterReportInfoAnnc, waterMeterReportInfoInst | waITe |
| waterMeterAlarm |  | waMAm |
| waterMeterReportInfo |  | wMRIo |
| waterMeterSetting |  | waMSg |
| waterPressureInterval | waterMeterSetting, waterMeterSettingAnnc, waterMeterSettingInst | waPIl |
| waterQualityMonitor |  | waQMr |
| waterSensor |  | watSr |
| waterTemperatureInterval | waterMeterSetting, waterMeterSettingAnnc, waterMeterSettingInst | waTIl |
| waterTemperatureSensorFault | waterMeterAlarm, waterMeterAlarmAnnc, waterMeterAlarmInst | wTSFt |
| weight | weightAnnc, weightInst, features, featuresAnnc, featuresInst | weigt |
| windDirection | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | winDn |
| windSpeed | airQualitySensor, airQualitySensorAnnc, airQualitySensorInst | winSd |
| withdrawalStatus | billWithdrawal, billWithdrawalAnnc, billWithdrawalInst | witSs |
| writable | dmStorage, dmStorageAnnc, dmStorageInst | write |
| writeIO |  | wriIO |
| writeSpeed | dmStorage, dmStorageAnnc, dmStorageInst | wriSd |
| zn | waterQualityMonitor, waterQualityMonitorAnnc, waterQualityMonitorInst | zn |

### 6.3.3 Void

### 6.3.4 Void

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

###

### \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End of Change 1 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*