|  |
| --- |
| CHANGE REQUEST |
| Meeting ID:\* |  |
| Source:\* |  |
| Date:\* |  |
| Reason for Change/s:\* |  |
| CR against: Release\* |  |
| CR against: WI\* | [x]  Active <#WI#> [ ]  MNT maintenance / < Work Item number(optional)>Is this a mirror CR? Yes [ ]  No [x] mirror CR number: [ ]  STE Small Technical Enhancements / < Work Item number (optional)>Only ONE of the above shall be ticked |
| CR against: TS/TR\* |  |
| Clauses \* |  |
| Type of change: \* | [ ]  Editorial change[x]  Bug Fix or Correction[ ]  Change to existing feature or functionality[ ]  New feature or functionalityOnly ONE of the above shall be ticked |
| Other TS/TR(s) impacted | None |
| Post Freeze checking:\* | This CR contains only essential changes and corrections? YES [x]  NO [ ] This CR may break backwards compatibility with the last approved version of the TS? YES [ ]  NO [ ]  |
| Template Version: January 2019 (do not modify) |

**oneM2M Notice**

The document to which this cover statement is attached is submitted to oneM2M. Participation in, or attendance at, any activity of oneM2M, constitutes acceptance of and agreement to be bound by terms of the Working Procedures and the Partnership Agreement, including the Intellectual Property Rights (IPR) Principles Governing oneM2M Work found in Annex 1 of the Partnership Agreement.

GUIDELINES for Change Requests:

Provide an informative introduction containing the problem(s) being solved, and a summary list of proposals.

Each CR should contain changes related to only one particular issue/problem.

In case of a correction, and the change apply to previous releases, a separate “mirror CR” should be posted at the same time of this CR

Mirror CR: applies only when the text, including clause numbering are exactly the same.

Companion CR: applies when the change means the same but the baselines differ in some way (e.g. clause number).

Follow the principle of completeness, where all changes related to the issue or problem within a deliverable are simultaneously proposed to be made E.g. A change impacting 5 tables should not only include a proposal to change only 3 tables. Includes any changes to references, definitions, and acronyms in the same deliverable.

Follow the drafting rules.

All pictures must be editable.

Check spelling and grammar to the extent practicable.

Use Change bars for modifications.

The change should include the current and surrounding clauses to clearly show where a change is located and to provide technical context of the proposed change. Additions of complete clauses need not show surrounding clauses as long as the proposed clause number clearly shows where the new clause is proposed to be located.

Multiple changes in a single CR shall be clearly separated by horizontal lines with embedded text such as, start of change 1, end of change 1, start of new clause, end of new clause.

When subsequent changes are made to content of a CR, then the accepted version should not show changes over changes. The accepted version of the CR should only show changes relative to the baseline approved text.

## Introduction

Adding short names for crossingBarrier MC

<https://git.onem2m.org/specifications/ts/ts-0023/-/merge_requests/43>

<https://git.onem2m.org/specifications/ts/ts-0023/-/merge_requests/43/diffs?commit_id=69a7771c00d3ee84ad6e63b4604f1ba637eeeb84>

----------------------- Start of change 1 -----------------------

---a/TS-0023-SDT\_based\_Information\_Model\_and\_Mapping\_for\_Vertical\_Industries.md
+++b/TS-0023-SDT\_based\_Information\_Model\_and\_Mapping\_for\_Vertical\_Industries.md

@@ -2313,9 +2313,6 @@ This ModuleClass displays a signal (e.g. direction arrow) to indicate a gate is

#### 5.3.1.115 crossingBarrier

An active barrier is used to block a pedestrian or vehicle from a control point (e.g. entrance and gate).

<mark>Editor note: the following attributes are missing from the short name tables in 6.3</mark>

\*\*Table 5.3.1.115-1: DataPoints of crossingBarrier ModuleClass\*\*

|Name |Type |R/W |Optional |Unit |Documentation |

@@ -2325,8 +2322,6 @@ An active barrier is used to block a pedestrian or vehicle from a control point

|timer |xs:time |RW |true | |The timer indicates the duration of barrierStatus is changed. This means that barrierStatus is set to the current value of barrierDefault. |

#### 5.3.1.116 threeDDisplay

This ModuleClass provides capabilities to give the information of a 3D display.

@@ -6054,6 +6049,8 @@ In protocol bindings resource attributes names for data points of module classes

|availableChannels |[televisionChannel](#53186-televisionchannel) |avaCs |

|backoffTime |[periodicalReportConfig](#53163-periodicalreportconfig) |bacTe |

|balance |[billDeposit](#531108-billdeposit), [billWithdrawal](#531109-billwithdrawal), [cashDispenser](#531111-cashdispenser), [coinDeposit](#531110-coindeposit), [prePaidCardReader](#531107-prepaidcardreader) |balae |

|barrierDefault |[crossingBarrier](#531115-crossingbarrier) |barDt |

|barrierStatus |[crossingBarrier](#531115-crossingbarrier) |barSs |

|basalMetabolism |[bodyCompositionAnalyser](#53114-bodycompositionanalyser) |basMm |

|bath |[hotWaterSupply](#53146-hotwatersupply) |bath |

|batteryThreshold |[battery](#53110-battery) |batTd |

@@ -6432,6 +6429,7 @@ In protocol bindings resource attributes names for data points of module classes

|textMessage |[textMessage](#53189-textmessage) |texMe |

|time |[keepWarm](#53148-keepwarm) |time |

|timePlanStatus |[slcParameterSetting](#53180-slcparametersetting) |tiPSs |

|timer |[crossingBarrier](#531115-crossingbarrier) |timer |

|timeRange |[slcParameterSetting](#53180-slcparametersetting) |timRe |

|timeRangeCount |[slcParameterSetting](#53180-slcparametersetting) |tiRCt |

|timeRangeLightDimmingValue |[slcParameterSetting](#53180-slcparametersetting) |tRLDV |

----------------------- End of change 1 -----------------------