|  |
| --- |
| CHANGE REQUEST |
| Meeting ID:\* |  |
| Source:\* |  |
| Date:\* |  |
| Reason for Change/s:\* |  |
| CR against: Release\* |  |
| CR against: WI\* | [x]  Active <#WI#> [ ]  MNT maintenance / < Work Item number(optional)>Is this a mirror CR? Yes [ ]  No [x] mirror CR number: [ ]  STE Small Technical Enhancements / < Work Item number (optional)>Only ONE of the above shall be ticked |
| CR against: TS/TR\* |  |
| Clauses \* |  |
| Type of change: \* | [ ]  Editorial change[x]  Bug Fix or Correction[ ]  Change to existing feature or functionality[ ]  New feature or functionalityOnly ONE of the above shall be ticked |
| Other TS/TR(s) impacted | None |
| Post Freeze checking:\* | This CR contains only essential changes and corrections? YES [x]  NO [ ] This CR may break backwards compatibility with the last approved version of the TS? YES [ ]  NO [ ]  |
| Template Version: January 2019 (do not modify) |

**oneM2M Notice**

The document to which this cover statement is attached is submitted to oneM2M. Participation in, or attendance at, any activity of oneM2M, constitutes acceptance of and agreement to be bound by terms of the Working Procedures and the Partnership Agreement, including the Intellectual Property Rights (IPR) Principles Governing oneM2M Work found in Annex 1 of the Partnership Agreement.

GUIDELINES for Change Requests:

Provide an informative introduction containing the problem(s) being solved, and a summary list of proposals.

Each CR should contain changes related to only one particular issue/problem.

In case of a correction, and the change apply to previous releases, a separate “mirror CR” should be posted at the same time of this CR

Mirror CR: applies only when the text, including clause numbering are exactly the same.

Companion CR: applies when the change means the same but the baselines differ in some way (e.g. clause number).

Follow the principle of completeness, where all changes related to the issue or problem within a deliverable are simultaneously proposed to be made E.g. A change impacting 5 tables should not only include a proposal to change only 3 tables. Includes any changes to references, definitions, and acronyms in the same deliverable.

Follow the drafting rules.

All pictures must be editable.

Check spelling and grammar to the extent practicable.

Use Change bars for modifications.

The change should include the current and surrounding clauses to clearly show where a change is located and to provide technical context of the proposed change. Additions of complete clauses need not show surrounding clauses as long as the proposed clause number clearly shows where the new clause is proposed to be located.

Multiple changes in a single CR shall be clearly separated by horizontal lines with embedded text such as, start of change 1, end of change 1, start of new clause, end of new clause.

When subsequent changes are made to content of a CR, then the accepted version should not show changes over changes. The accepted version of the CR should only show changes relative to the baseline approved text.

## Introduction

Adding short names for emergencyHandler MC

<https://git.onem2m.org/specifications/ts/ts-0023/-/merge_requests/52>

<https://git.onem2m.org/specifications/ts/ts-0023/-/merge_requests/52/diffs?commit_id=949453fb13cee3674077a7959692f0bf4c30702e>

----------------------- Start of change 1 -----------------------

---a/TS-0023-SDT\_based\_Information\_Model\_and\_Mapping\_for\_Vertical\_Industries.md
+++b/TS-0023-SDT\_based\_Information\_Model\_and\_Mapping\_for\_Vertical\_Industries.md

@@ -2560,7 +2560,6 @@ This ModuleClass provides the capability of creating oneM2M based information fr

#### 5.3.10.2 emergencyHandler

This ModuleClass provides the capability of triggering things to change into an emergency mode and of enabling things to identify whether an event described in oneM2M based information that is received from Public Warning Center (MN) is relevant to things. If any change happens in received warning messages such as updating oneM2M based information and cancelling the dissemination of oneM2M based information of previously received public warning messages, this ModuleClass updates oneM2M based information corresponding to those received public warning messages to control behaviour of things.

\*\*Table 5.3.10.2-1: DataPoints of emergencyHandler ModuleClass\*\*

|Name |Type |R/W |Optional |Unit |Documentation |

@@ -2584,8 +2583,6 @@ This ModuleClass provides the capability of triggering things to change into an

|areaRadius |xs:float |RW |true |m |The radius of the affected area location. |

#### 5.3.10.3 settings

This ModuleClass provides the capability of selecting the option that allows things to decide to take action as receiving oneM2M based information of public warning messages.

@@ -6047,6 +6044,9 @@ In protocol bindings resource attributes names for data points of module classes

|algae |[waterQualityMonitor](#53198-waterqualitymonitor) |algae |

|altitude |[geoLocation](#53141-geolocation) |altie |

|anionics |[waterQualityMonitor](#53198-waterqualitymonitor) |anios |

|areaLatitude |[emergencyHandler](#53102-emergencyhandler) |areLe |

|areaLongitude |[emergencyHandler](#53102-emergencyhandler) |areL0 |

|areaRadius |[emergencyHandler](#53102-emergencyhandler) |areRs |

|aroh |[waterQualityMonitor](#53198-waterqualitymonitor) |aroh |

|as |[waterQualityMonitor](#53198-waterqualitymonitor) |as |

|atmosphericPressure |[barometer](#531101-barometer) |atmPe |

@@ -6070,6 +6070,7 @@ In protocol bindings resource attributes names for data points of module classes

|capacity |[battery](#53110-battery) |capay |

|cd |[waterQualityMonitor](#53198-waterqualitymonitor) |cd |

|cellID |[connectivity](#53125-connectivity) |celID |

|certainty |[emergencyHandler](#53102-emergencyhandler) |certy |

|ch2o |[airQualitySensor](#5316-airqualitysensor) |ch2o |

|channelId |[televisionChannel](#53186-televisionchannel) |chaId |

|channelName |[televisionChannel](#53186-televisionchannel) |chaNe |

@@ -6148,10 +6149,14 @@ In protocol bindings resource attributes names for data points of module classes

|do |[waterQualityMonitor](#53198-waterqualitymonitor) |do |

|doorState |[doorStatus](#53130-doorstatus) |dooSe |

|duration |[overcurrentSensor](#53158-overcurrentsensor), [recorder](#53170-recorder) |dur |

|effective |[emergencyHandler](#53102-emergencyhandler) |effee |

|electricEnergy |[battery](#53110-battery) |eleEy |

|emergencyMode |[emergencyHandler](#53102-emergencyhandler) |emeMe |

|enabled |[dmEventLog](#587-dmeventlog) |enabd |

|energy |[pulsemeter](#53168-pulsemeter) |enery |

|estimatedTimeToEnd |[timer](#53190-timer) |eTTEd |

|eventCodes |[emergencyHandler](#53102-emergencyhandler) |eveCs |

|expires |[emergencyHandler](#53102-emergencyhandler) |expis |

|extraRinse |[clothesWasherJobModeOption](#53122-clotheswasherjobmodeoption) |extRe |

|f |[waterQualityMonitor](#53198-waterqualitymonitor) |f |

|fakeStatus |[billDeposit](#531108-billdeposit), [coinDeposit](#531110-coindeposit) |fakSs |

@@ -6192,6 +6197,7 @@ In protocol bindings resource attributes names for data points of module classes

|horizontalDirection |[airFlow](#5314-airflow) |horDn |

|humidity |[airQualitySensor](#5316-airqualitysensor) |humiy |

|hwVersion |[dmDeviceInfo](#583-dmdeviceinfo)|hweVn |

|identifier |[emergencyHandler](#53102-emergencyhandler) |idenr |

|impactDirectionHorizontal |[impactSensor](#53147-impactsensor) |imDHl |

|impactDirectionVertical |[impactSensor](#53147-impactsensor) |imDVl |

|impactLevel |[impactSensor](#53147-impactsensor) |impLl |

@@ -6275,6 +6281,7 @@ In protocol bindings resource attributes names for data points of module classes

|modality |[pulsemeter](#53168-pulsemeter) |moday |

|model |[dmDeviceInfo](#583-dmdeviceinfo) |model |

|monitoringEnabled |[airQualitySensor](#5316-airqualitysensor) |monEd |

|msgType |[emergencyHandler](#53102-emergencyhandler) |msgTe |

|multiFirmware |[dmFirmware](#585-dmfirmware) |mulFe |

|multiplyingFactors |[energyConsumption](#53132-energyconsumption), [energyGeneration](#53133-energygeneration) |mulFs |

|muscle |[bioElectricalImpedanceAnalysis](#53113-bioelectricalimpedanceanalysis) |musce |

@@ -6293,6 +6300,7 @@ In protocol bindings resource attributes names for data points of module classes

|odor |[airQualitySensor](#5316-airqualitysensor) |odor |

|oil |[waterQualityMonitor](#53198-waterqualitymonitor) |oil |

|onlineStatus |[slcReportInfo](#53181-slcreportinfo) |onlSs |

|onset |[emergencyHandler](#53102-emergencyhandler) |onset |

|openAlarm |[doorStatus](#53130-doorstatus) |opeAm |

|openDuration |[doorStatus](#53130-doorstatus) |opeDn |

|openLevel |[openLevel](#53156-openlevel) |opeLl |

@@ -6352,6 +6360,7 @@ In protocol bindings resource attributes names for data points of module classes

|rechargeGas |[gasChargingControl](#53138-gaschargingcontrol) |recGs |

|recipientID |[phoneCall](#53164-phonecall) |recID |

|red |[colour](#53123-colour) |red |

|references |[emergencyHandler](#53102-emergencyhandler) |refes |

|referenceTimer |[timer](#53190-timer) |refTr |

|relativeHumidity |[relativeHumidity](#53172-relativehumidity) |relHy |

|reliability |[features](#5391-features) |reliy |

@@ -6377,8 +6386,11 @@ In protocol bindings resource attributes names for data points of module classes

|secondaryUrl |[dmFirmware](#585-dmfirmware) |secUl |

|secondaryVersion |[dmFirmware](#585-dmfirmware) |secVn |

|securityModes |[securityMode](#53176-securitymode) |secMs |

|sender |[emergencyHandler](#53102-emergencyhandler) |sendr |

|sensitivity |[motionSensor](#53154-motionsensor) |sensy |

|sent |[emergencyHandler](#53102-emergencyhandler) |sent |

|serialNumber |[dmDeviceInfo](#583-dmdeviceinfo) |serNr |

|severity |[emergencyHandler](#53102-emergencyhandler) |sevey |

|signalECL |[connectivity](#53125-connectivity) |siECL |

|significantDigits |[energyConsumption](#53132-energyconsumption), [energyGeneration](#53133-energygeneration) |sigDs |

|silentTime |[motionSensor](#53154-motionsensor) |silTe |

@@ -6397,7 +6409,7 @@ In protocol bindings resource attributes names for data points of module classes

|standardreferenceVoltage |[slcAlarm](#53179-slcalarm) |staVe |

|startPause |[operationMode](#53157-operationmode) |staPe |

|state |[dmAgent](#582-dmagent), [dmPackage](#588-dmpackage), [dmFirmware](#585-dmfirmware), [binarySwitch](#53112-binaryswitch) |state |

|status |[boiler](#53115-boiler), [dmEventLog](#587-dmeventlog), [electricVehicleConnector](#53131-electricvehicleconnector), [faultDetection](#53134-faultdetection), filterInf, [mediaSelect](#53153-mediaselect) |sus |

|status |[boiler](#53115-boiler), [dmEventLog](#587-dmeventlog), [electricVehicleConnector](#53131-electricvehicleconnector), [emergencyHandler](#53102-emergencyhandler), [faultDetection](#53134-faultdetection), <mark>Editor note: check attribute</mark> filterInf, [mediaSelect](#53153-mediaselect) |sus |

|steamTreat |[clothesWasherJobModeOption](#53122-clotheswasherjobmodeoption) |steTt |

|step |[numberValue](#53155-numbervalue) |step |

|stepValue |[audioVolume](#5318-audiovolume), [openLevel](#53156-openlevel), [temperature](#53187-temperature) |steVe |

@@ -6451,6 +6463,7 @@ In protocol bindings resource attributes names for data points of module classes

|underVoltagePercent |[slcAlarm](#53179-slcalarm) |unVPt |

|underVoltageThreshold |[slcAlarm](#53179-slcalarm) |unVTd |

|unit |[temperature](#53187-temperature), [temperatureAlarm](#53188-temperaturealarm) |unit |

|urgency |[emergencyHandler](#53102-emergencyhandler) |urgey |

|urgencyButtonPush |[waterMeterAlarm](#53194-watermeteralarm)|urBPh |

|uri |[printQueue](#53167-printqueue) |ur0 |

|url |[sessionDescription](#53177-sessiondescription), [dmPackage](#588-dmpackage), [dmSoftware](#586-dmsoftware) |url |

----------------------- End of change 1 -----------------------