|  |
| --- |
|  |

|  |  |
| --- | --- |
| CHANGE REQUEST | |
| Meeting ID:\* | SDS #52 |
| Source:\* | Andreas Kraft, DT, [A.Kraft@telekom.de](mailto:A.Kraft@telekom.de)  Andreas Neubacher, DT, [Andreas.Neubacher@magenta.at](mailto:Andreas.Neubacher@magenta.at) |
| Date:\* | 2022-01-20 |
| Reason for Change/s:\* | Adding [credentials] specialization to TS-0022 (TS-0001) |
| CR against: Release\* | Release 5 |
| CR against: WI\* | Active WI-xxxx  MNT maintenance / < Work Item number(optional)>  Is this a mirror CR? Yes  No  mirror CR number: (Note to Rapporteur - use latest agreed revision)  STE Small Technical Enhancements / < Work Item number (optional)>  Only ONE of the above shall be ticked |
| CR against: TS/TR\* | TS-0001, V4.13.0 |
| Clauses \* | TS-0001: 9.6.1.2.1 |
| Type of change: \* | Editorial change  Bug Fix or Correction  Change to existing feature or functionality  New feature or functionality  Only ONE of the above shall be ticked |
| Impacted other TS/TR(s) |  |
| Post Freeze checking:\* | This CR contains only essential changes and corrections? YES  NO  This CR may break backwards compatibility with the last approved version of the TS? YES  NO |
| Template Version: January 2017 (Do not modify) | |

**oneM2M Notice**

The document to which this cover statement is attached is submitted to oneM2M. Participation in, or attendance at, any activity of oneM2M, constitutes acceptance of and agreement to be bound by terms of the Working Procedures and the Partnership Agreement, including the Intellectual Property Rights (IPR) Principles Governing oneM2M Work found in Annex 1 of the Partnership Agreement.

GUIDELINES for Change Requests:

Provide an informative introduction containing the problem(s) being solved, and a summary list of proposals.

Each CR should contain changes related to only one particular issue/problem.

In case of a correction, and the change apply to previous releases, a separate “mirror CR” should be posted at the same time of this CR

Mirror CR: applies only when the text, including clause numbering are exactly the same.

Companion CR: applies when the change means the same but the baselines differ in some way (e.g. clause number).

Follow the principle of completeness, where all changes related to the issue or problem within a deliverable are simultaneously proposed to be made E.g. A change impacting 5 tables should not only include a proposal to change only 3 tables. Includes any changes to references, definitions, and acronyms in the same deliverable.

Follow the drafting rules.

All pictures must be editable.

Check spelling and grammar to the extent practicable.

Use Change bars for modifications.

The change should include the current and surrounding clauses to clearly show where a change is located and to provide technical context of the proposed change. Additions of complete clauses need not show surrounding clauses as long as the proposed clause number clearly shows where the new clause is proposed to be located.

Multiple changes in a single CR shall be clearly separated by horizontal lines with embedded text such as, start of change 1, end of change 1, start of new clause, end of new clause.


When subsequent changes are made to content of a CR, then the accepted version should not show changes over changes. The accepted version of the CR should only show changes relative to the baseline approved text.

Introduction

This CR proposes a new <mgmtObj> specialization to store general credentials for a device.

In addition to, for example, network identification and authentication, a device might also need credentials to authenticate with third party components such as message broker or an additional non-oneM2M backend components which are out-of-scope of the common oneM2M Mca communication specification. Beside the already available specializations, for example for OAuth2, storing simple username/password combinations or tokens are currently not supported. Though it is recommended to utilize more modern authentication schemes, basic or token-based authentication is still widely used in legacy installations, and in installations that cannot afford or utilize an operated trust infrastructure.

The following diagram shows the general flow. An AE on an ADN requires credentials to access services on a non-oneM2M service. A CSE stores the credentials for that ADN together with other management information and makes them available via Mca. The usual oneM2M security and access methods do apply here, though an implementation may choose to store credentials in a more secure way.



A similar <flexContainer> specialization is specified in TS-0023, 5.3.1.27 “credentials”. That specialization may be added or referenced to <flexContainer> - based device management in TS-0023 to provide the same functionality as well. This would be for another CR.

This is a mirror CR for SDS-2021-0185R01-Adding\_[credentials]\_specialization\_to\_TS-0022 for TS-0004

Change 1 provides an update of TS-0001, Table 9.6.1.2.1-1: <mgmtObj> Specializations.

Question: The TS-0022 mgmtObj specializations are not listed in TS-0001, Table 9.6.18-1: Child resources of <node> resource. But where are they, e.g. to state the cardinality.

### \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Start of Change 1 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

##### 9.6.1.2.1 Specializations of <*mgmtObj*>

Table 9.6.1.2.1-1 lists specializations of the *<mgmtObj>* resource type in which the *mgmtDefinition* attribute contains an enumerated value that provides further definition of the resource.

Table 9.6.1.2.1-1: <*mgmtObj*> Specializations

| Resource specialization | Short Description | Child Resource Types | Parent Resource Types | Clause |
| --- | --- | --- | --- | --- |
| *activeCmdhPolicy* | Provides a link to the currently active set of CMDH policies | None specified | *node* | D.12.1 |
| *areaNwkDeviceInfo* | Provides information about the Node in the M2M Area Network | *subscription* | *node* | D.6 |
| *areaNwkInfo* | Describes the list of Nodes attached behind the MN node and its physical or underlying relation among the nodes in the M2M Area Network | *subscription* | *node* | D.5 |
| *battery* | Provides the power information of the node (e.g. remaining battery charge) | *subscription* | *node* | D.7 |
| *cmdhBuffer* | Defines CMDH buffer usage limits | *subscription* | *cmdhPolicy* | D.12.8 |
| *cmdhDefaults* | Defines CMDH default values | *cmdhDefEcValue, cmdhEcDefParamValues*  *subscription* | *cmdhPolicy* | D.12.2 |
| *cmdhEcDefParamValues* | Represent a specific set of default values for the CMDH related parameters | *subscription* | *cmdhDefaults* | D.12.4 |
| *cmdhDefEcValue* | Defines a value for the ***Event Category*** parameter of an incoming request when it is not defined | *subscription* | *cmdhDefaults* | D.12.3 |
| *cmdhLimits* | Defines limits for CMDH related parameter values | *subscription* | *cmdhPolicy* | D.12.5 |
| *cmdhNetworkAccessRules* | Defines rules for the usage of underlying networks | *cmdhNwAccessRule,*  *subscription* | *cmdhPolicy* | D.12.6 |
| *cmdhNwAccessRule* | Defines a rule for the usage of underlying networks | *subscription* | *cmdhNetworkAccessRules* | D.12.7 |
| *cmdhPolicy* | A set of rules defining which CMDH parameters will be used by default | *cmdhDefaults, cmdhLimits, cmdhNetworkAccessRules, cmdhBuffer,*  *subscription* | *node* | D.12 |
| *deviceCapability* | Contains information about the capability supported by the Node | *subscription* | *node* | D.9 |
| *deviceInfo* | Contains information about the identity, manufacturer and model number of the device | *subscription* | *node* | D.8 |
| *eventLog* | Contains information about the log of events of the Node | *subscription* | *node* | D.11 |
| *firmware* | Provides information about the firmware of the Node (e.g. name, version) | *subscription* | *node* | D.2 |
| *memory* | Provides the memory (typically RAM) information of the node (e.g. the amount of total volatile memory) | *subscription* | *node* | D.4 |
| *reboot* | Used to reboot or reset the Node | *subscription* | *node* | D.10 |
| *software* | Provides information about the software of the Node | *subscription* | *node* | D.3 |
| *registration* | To convey the service layer configuration information | *subscription* | *node* | 7.1 in [10] |
| *dataCollection* | To convey the application configuration information | *subscription* | *node* | 7.2 in [10] |
| *authenticationProfile* | To convey the configuration information regarding establishing mutually-authenticated secure communications | *subscription* | *node* | 7.1 in [10] |
| *myCertFileCred* | To configure a certificate or certificate chain | *subscription* | *authenticationProfile* | 7.1 in [10] |
| *trustAnchorCred* | To identify a trust anchor certificate for validation of certificates | *subscription* | *authenticationProfile* | 7.1 in [10] |
| *MAFClientRegCfg* | To convey instructions regarding the MAF Client Registration procedure | *subscription* | *authenticationProfile* | 7.1 in [10] |
| *wifiClient* | To set up configuration of WiFi connection on the client device. | *subscription* | *node* | 7.1 in [10] |
| *storage* | To manage available storage memory on the device | *subscription* | *node* | D.13 |
| *OAuth2Authentication* | To store access token and refresh token used in OAuth2 security protocol | *subscription* | *node* | 7.1 in [10] |
| *credentials* | To store credentials on the client device for authentications | *Subscription* | *node* | 7.1 in [10] |

### \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End of Change 1 \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*