|  |
| --- |
|  |

|  |
| --- |
| CHANGE REQUEST |
| Meeting ID:\* | RDM#39 |
| Source:\* | niuyawen, niuyawen@chinamobile.com |
| Date:\* | 2019-01-18 |
| Reason for Change/s:\* | Adding a new element for Interpretation of enumCallSate Enumeration type definitions |
| CR against: Release\* | Rel.4  |
| CR against: WI\* | [x]  Active WI-0017[ ]  MNT maintenance / < Work Item number(optional)>Is this a mirror CR? Yes [ ]  No [ ] mirror CR number: (Note to Rapporteur - use latest agreed revision)[ ]  STE Small Technical Enhancements / < Work Item number (optional)>Only ONE of the above shall be ticked |
| CR against: TS/TR\* | TS-0023 V4.0.0 |
| Clauses \* | New clauses in 5.6.6 |
| Type of change: \* | [ ]  Editorial change[ ]  Bug Fix or Correction[ ]  Change to existing feature or functionality[x]  New feature or functionalityOnly ONE of the above shall be ticked |
| Impacted other TS/TR(s) |  |
| Post Freeze checking:\* | This CR contains only essential changes and corrections? YES [x]  NO [ ] This CR may break backwards compatibility with the last approved version of the TS? YES [ ]  NO [x]  |
| Template Version: January 2017 (Do not modify) |

**oneM2M Notice**

The document to which this cover statement is attached is submitted to oneM2M. Participation in, or attendance at, any activity of oneM2M, constitutes acceptance of and agreement to be bound by terms of the Working Procedures and the Partnership Agreement, including the Intellectual Property Rights (IPR) Principles Governing oneM2M Work found in Annex 1 of the Partnership Agreement.

## Introduction

This CR introduces a new element for Interpretation of enumCallSate Enumeration type definitions.

### -----------------------Start of change 1-------------------------------------------

### 5.6.6 hd:enumCallState

Used for the “callState” data point in the “phoneCall” ModuleClass.

Table ‑: Interpretation of hd:enumCallState

|  |  |  |
| --- | --- | --- |
| Value | Interpretation | Note |
| 1 | hangup |  |
| 2 | calling |  |
| 3 | ringing |  |
| 4 | busy |  |
| 5 | answered |  |
| 6 | noline |  |
| 7 | voicemail |  |
| 8 | redirected |  |
| NOTE: See clause 5.3.56 “phoneCall” |

### -----------------------End of change 1---------------------------------------------